<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.0">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting keepoldvectorfont="yes"/>
<setting verticaltext="up"/>
</settings>
<grid distance="50" unitdist="mil" unit="mil" style="lines" multiple="1" display="yes" altdistance="5" altunitdist="mil" altunit="mil"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="no" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="no" active="yes"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="no" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="no" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="no" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="no" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="no" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="no" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="no" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="no" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="no" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="yes" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="no" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="no" active="yes"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="no" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="yes" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
<layer number="4" name="Route4" color="1" fill="4" visible="no" active="no"/>
<layer number="5" name="Route5" color="4" fill="4" visible="no" active="no"/>
<layer number="6" name="Route6" color="1" fill="8" visible="no" active="no"/>
<layer number="7" name="Route7" color="4" fill="8" visible="no" active="no"/>
<layer number="8" name="Route8" color="1" fill="2" visible="no" active="no"/>
<layer number="9" name="Route9" color="4" fill="2" visible="no" active="no"/>
<layer number="10" name="Route10" color="1" fill="7" visible="no" active="no"/>
<layer number="11" name="Route11" color="4" fill="7" visible="no" active="no"/>
<layer number="12" name="Route12" color="1" fill="5" visible="no" active="no"/>
<layer number="13" name="Route13" color="4" fill="5" visible="no" active="no"/>
<layer number="14" name="Route14" color="1" fill="6" visible="no" active="no"/>
<layer number="15" name="Route15" color="4" fill="6" visible="no" active="no"/>
<layer number="2" name="Route2" color="1" fill="3" visible="no" active="no"/>
<layer number="3" name="Route3" color="4" fill="3" visible="no" active="no"/>
</layers>
<library>
<description>Inductors by NKL® 

        _/_/            _/          _/          _/          _/
      _/   _/         _/          _/     _/               _/
    _/      _/      _/          _/_/                    _/
  _/         _/   _/          _/     _/               _/
_/            _/_/          _/          _/          _/ _/ _/ _/ _/

http://www.nkl-emv.de

Allgemeine Informationen:
- können die Pinanschlüsse in Becher- und Sockelversionen, kundenspezifisch, geändert werden; (-&gt;Absprache mit NKL®)
- sind die Rastermaße nackter Drosseln nur Vorschläge; Layouts für nackte, mehrphasige, Drosseln, in liegender Bauweise,
  sind nicht erfasst, sondern müssen vom Anwender gemäß Muster entworfen werden;
- sollte die Auswahl eines Bauteils mit NKL® abgesprochen werden, da bestimmte Kombinationen (Drossel - Becher - Strom)
   unwirtschaftlich bzw. nicht produzierbar sind;

Generally,
- the contacts of cup devices may be selected inividually however only in consultation with NKL®;
- grid pinning dimensions of plain chokes are only suggested; layouts for plain, multiphase, flat built in chokes, are not included
   and need to be designed by the customer according to a sample;
- the final selection of a device should be in agreement with NKL® since some combinations (regarding choke, package and current)
   may be uneconomical or even not producible;

Please contact us for more information:

	NKL GmbH
	Birkichstr. 15
	74549 Wolpertshausen

	Tel:  +49 (0)7904 9781-0
	Fax:  +49 (0)7904 9781-50

CadSoft and the author do not warrant that this library is error free or will meet someones specific requirements.

Created by Michael.Fuchshuber@nkl-emv.de
NKL® 07/42</description>
<packages>
<package name="B1">
<description>Becher B1 (cup B1)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 19x10(12.5)x19
RM (grid): (12.5x10)mm
manufactured by NKL®</description>
<wire x1="-9.5" y1="5" x2="-8" y2="5" width="0.127" layer="21"/>
<wire x1="-8" y1="5" x2="-7" y2="6.5" width="0.127" layer="51"/>
<wire x1="-7" y1="6.5" x2="-5.5" y2="6.5" width="0.127" layer="51"/>
<wire x1="-5.5" y1="6.5" x2="-4.5" y2="5" width="0.127" layer="51"/>
<wire x1="-4.5" y1="5" x2="4.5" y2="5" width="0.127" layer="21"/>
<wire x1="4.5" y1="5" x2="5.5" y2="6.5" width="0.127" layer="51"/>
<wire x1="5.5" y1="6.5" x2="7" y2="6.5" width="0.127" layer="51"/>
<wire x1="7" y1="6.5" x2="8" y2="5" width="0.127" layer="51"/>
<wire x1="8" y1="5" x2="9.5" y2="5" width="0.127" layer="21"/>
<wire x1="9.5" y1="5" x2="9.5" y2="-5" width="0.127" layer="21"/>
<wire x1="9.5" y1="-5" x2="8" y2="-5" width="0.127" layer="21"/>
<wire x1="8" y1="-5" x2="7" y2="-6.5" width="0.127" layer="51"/>
<wire x1="7" y1="-6.5" x2="5.5" y2="-6.5" width="0.127" layer="51"/>
<wire x1="5.5" y1="-6.5" x2="4.5" y2="-5" width="0.127" layer="51"/>
<wire x1="4.5" y1="-5" x2="-4.5" y2="-5" width="0.127" layer="21"/>
<wire x1="-4.5" y1="-5" x2="-5.5" y2="-6.5" width="0.127" layer="51"/>
<wire x1="-5.5" y1="-6.5" x2="-7" y2="-6.5" width="0.127" layer="51"/>
<wire x1="-7" y1="-6.5" x2="-8" y2="-5" width="0.127" layer="51"/>
<wire x1="-8" y1="-5" x2="-9.5" y2="-5" width="0.127" layer="21"/>
<wire x1="-9.5" y1="-5" x2="-9.5" y2="5" width="0.127" layer="21"/>
<pad name="2" x="-6.25" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="6.25" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="6.25" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="1" x="-6.25" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-5.08" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B2">
<description>Becher B2 (cup B2)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 22x10(12.5)x22
RM (grid): (12.5x10)mm
manufactured by NKL®</description>
<wire x1="-11" y1="5" x2="-8" y2="5" width="0.127" layer="21"/>
<wire x1="-8" y1="5" x2="-7" y2="6.25" width="0.127" layer="51"/>
<wire x1="-7" y1="6.25" x2="-5.5" y2="6.25" width="0.127" layer="51"/>
<wire x1="-5.5" y1="6.25" x2="-4.5" y2="5" width="0.127" layer="51"/>
<wire x1="-4.5" y1="5" x2="4.5" y2="5" width="0.127" layer="21"/>
<wire x1="4.5" y1="5" x2="5.5" y2="6.25" width="0.127" layer="51"/>
<wire x1="5.5" y1="6.25" x2="7" y2="6.25" width="0.127" layer="51"/>
<wire x1="7" y1="6.25" x2="8" y2="5" width="0.127" layer="51"/>
<wire x1="8" y1="5" x2="11" y2="5" width="0.127" layer="21"/>
<wire x1="11" y1="5" x2="11" y2="-5" width="0.127" layer="21"/>
<wire x1="11" y1="-5" x2="8" y2="-5" width="0.127" layer="21"/>
<wire x1="8" y1="-5" x2="7" y2="-6.25" width="0.127" layer="51"/>
<wire x1="7" y1="-6.25" x2="5.5" y2="-6.25" width="0.127" layer="51"/>
<wire x1="5.5" y1="-6.25" x2="4.5" y2="-5" width="0.127" layer="51"/>
<wire x1="4.5" y1="-5" x2="-4.5" y2="-5" width="0.127" layer="21"/>
<wire x1="-4.5" y1="-5" x2="-5.5" y2="-6.25" width="0.127" layer="51"/>
<wire x1="-5.5" y1="-6.25" x2="-7" y2="-6.25" width="0.127" layer="51"/>
<wire x1="-7" y1="-6.25" x2="-8" y2="-5" width="0.127" layer="51"/>
<wire x1="-8" y1="-5" x2="-11" y2="-5" width="0.127" layer="21"/>
<wire x1="-11" y1="-5" x2="-11" y2="5" width="0.127" layer="21"/>
<pad name="1" x="-6.25" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="-6.25" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="6.25" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="6.25" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-5.08" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B71">
<description>Becher B7 (cup B7)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 18(20)x9
RM (grid) [mm]: 10x15 / 5x17.5
manufactured by NKL®</description>
<wire x1="6.5" y1="-6" x2="6.5" y2="-8" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-8" x2="6.5" y2="-8" width="0.127" layer="51" curve="71.675306"/>
<wire x1="-6.5" y1="8" x2="6.5" y2="8" width="0.127" layer="51" curve="-71.675306"/>
<wire x1="-6.5" y1="-6" x2="-6.5" y2="6" width="0.127" layer="21" curve="-85.41878"/>
<wire x1="-6.5" y1="6" x2="-6.5" y2="8" width="0.127" layer="21"/>
<wire x1="6.5" y1="6" x2="6.5" y2="8" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-8" x2="-6.5" y2="-6" width="0.127" layer="21"/>
<wire x1="6.5" y1="6" x2="6.5" y2="-6" width="0.127" layer="21" curve="-85.41878"/>
<pad name="3" x="5" y="7.5" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="1" x="-5" y="7.5" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="2" x="-5" y="-7.5" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="4" x="5" y="-7.5" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="5" x="-2.5" y="8.75" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="7" x="2.5" y="8.75" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="6" x="-2.5" y="-8.75" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="8" x="2.5" y="-8.75" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<text x="-2.54" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B1/2">
<description>Becher B1/2 (cup B1/2)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 19x10(12.5)x19
RM (grid): (10x10)mm
manufactured by NKL®</description>
<wire x1="-9.25" y1="5" x2="-6.75" y2="5" width="0.127" layer="21"/>
<wire x1="-6.75" y1="5" x2="-6" y2="6.25" width="0.127" layer="51"/>
<wire x1="-6" y1="6.25" x2="-4" y2="6.25" width="0.127" layer="51"/>
<wire x1="-4" y1="6.25" x2="-3.25" y2="5" width="0.127" layer="51"/>
<wire x1="-3.25" y1="5" x2="3.25" y2="5" width="0.127" layer="21"/>
<wire x1="3.25" y1="5" x2="4" y2="6.25" width="0.127" layer="51"/>
<wire x1="4" y1="6.25" x2="6" y2="6.25" width="0.127" layer="51"/>
<wire x1="6" y1="6.25" x2="6.75" y2="5" width="0.127" layer="51"/>
<wire x1="6.75" y1="5" x2="9.25" y2="5" width="0.127" layer="21"/>
<wire x1="9.25" y1="5" x2="9.25" y2="-5" width="0.127" layer="21"/>
<wire x1="9.25" y1="-5" x2="6.75" y2="-5" width="0.127" layer="21"/>
<wire x1="6.75" y1="-5" x2="6" y2="-6.25" width="0.127" layer="51"/>
<wire x1="6" y1="-6.25" x2="4" y2="-6.25" width="0.127" layer="51"/>
<wire x1="4" y1="-6.25" x2="3.25" y2="-5" width="0.127" layer="51"/>
<wire x1="3.25" y1="-5" x2="-3.25" y2="-5" width="0.127" layer="21"/>
<wire x1="-3.25" y1="-5" x2="-4" y2="-6.25" width="0.127" layer="51"/>
<wire x1="-4" y1="-6.25" x2="-6" y2="-6.25" width="0.127" layer="51"/>
<wire x1="-6" y1="-6.25" x2="-6.75" y2="-5" width="0.127" layer="51"/>
<wire x1="-6.75" y1="-5" x2="-9.25" y2="-5" width="0.127" layer="21"/>
<wire x1="-9.25" y1="-5" x2="-9.25" y2="5" width="0.127" layer="21"/>
<pad name="2" x="-5" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="5" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="5" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="1" x="-5" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B5">
<description>Becher B5 (cup B5)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 13x6x14
RM (grid): (10x3)mm
manufactured by NKL®</description>
<wire x1="-6.5" y1="3" x2="6.5" y2="3" width="0.127" layer="21"/>
<wire x1="6.5" y1="3" x2="6.5" y2="-3" width="0.127" layer="51"/>
<wire x1="6.5" y1="-3" x2="-6.5" y2="-3" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-3" x2="-6.5" y2="3" width="0.127" layer="51"/>
<pad name="1" x="-5" y="1.5" drill="1.27" shape="long"/>
<pad name="2" x="-5" y="-1.5" drill="1.27" shape="long"/>
<pad name="4" x="5" y="-1.5" drill="1.27" shape="long"/>
<pad name="3" x="5" y="1.5" drill="1.27" shape="long"/>
<text x="-6.35" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.35" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B3">
<description>Becher B3 (cup B3)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 27x14(18)x27
RM (grid): (15x12.5)mm
manufactured by NKL®</description>
<wire x1="-13.5" y1="7" x2="-10" y2="7" width="0.127" layer="21"/>
<wire x1="-10" y1="7" x2="-8" y2="9" width="0.127" layer="21"/>
<wire x1="-8" y1="9" x2="-7" y2="9" width="0.127" layer="21"/>
<wire x1="-7" y1="9" x2="-5" y2="7" width="0.127" layer="21"/>
<wire x1="-5" y1="7" x2="5" y2="7" width="0.127" layer="21"/>
<wire x1="5" y1="7" x2="7" y2="9" width="0.127" layer="21"/>
<wire x1="7" y1="9" x2="8" y2="9" width="0.127" layer="21"/>
<wire x1="8" y1="9" x2="10" y2="7" width="0.127" layer="21"/>
<wire x1="10" y1="7" x2="13.5" y2="7" width="0.127" layer="21"/>
<wire x1="13.5" y1="7" x2="13.5" y2="-7" width="0.127" layer="21"/>
<wire x1="13.5" y1="-7" x2="10" y2="-7" width="0.127" layer="21"/>
<wire x1="10" y1="-7" x2="8" y2="-9" width="0.127" layer="21"/>
<wire x1="8" y1="-9" x2="7" y2="-9" width="0.127" layer="21"/>
<wire x1="7" y1="-9" x2="5" y2="-7" width="0.127" layer="21"/>
<wire x1="5" y1="-7" x2="-5" y2="-7" width="0.127" layer="21"/>
<wire x1="-5" y1="-7" x2="-7" y2="-9" width="0.127" layer="21"/>
<wire x1="-7" y1="-9" x2="-8.25" y2="-9" width="0.127" layer="21"/>
<wire x1="-8.25" y1="-9" x2="-10" y2="-7" width="0.127" layer="21"/>
<wire x1="-10" y1="-7" x2="-13.5" y2="-7" width="0.127" layer="21"/>
<wire x1="-13.5" y1="-7" x2="-13.5" y2="7" width="0.127" layer="21"/>
<pad name="1" x="-7.5" y="6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="-7.5" y="-6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="7.5" y="6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="7.5" y="-6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B4">
<description>Becher B4 (cup B4)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 32x18.5(22.5)x31
RM (grid): (17.5x12.5)mm
manufactured by NKL®</description>
<wire x1="-16" y1="9.25" x2="-9.25" y2="9.25" width="0.127" layer="21"/>
<wire x1="-9.25" y1="9.25" x2="-7" y2="11.5" width="0.127" layer="21"/>
<wire x1="-7" y1="11.5" x2="-5.5" y2="11.5" width="0.127" layer="21"/>
<wire x1="-5.5" y1="11.5" x2="-3.25" y2="9.25" width="0.127" layer="21"/>
<wire x1="-3.25" y1="9.25" x2="3.25" y2="9.25" width="0.127" layer="21"/>
<wire x1="3.25" y1="9.25" x2="5.5" y2="11.5" width="0.127" layer="21"/>
<wire x1="5.5" y1="11.5" x2="7" y2="11.5" width="0.127" layer="21"/>
<wire x1="7" y1="11.5" x2="9.25" y2="9.25" width="0.127" layer="21"/>
<wire x1="9.25" y1="9.25" x2="16" y2="9.25" width="0.127" layer="21"/>
<wire x1="16" y1="9.25" x2="16" y2="-9.25" width="0.127" layer="21"/>
<wire x1="16" y1="-9.25" x2="9.25" y2="-9.25" width="0.127" layer="21"/>
<wire x1="9.25" y1="-9.25" x2="7" y2="-11.5" width="0.127" layer="21"/>
<wire x1="7" y1="-11.5" x2="5.5" y2="-11.5" width="0.127" layer="21"/>
<wire x1="5.5" y1="-11.5" x2="3.25" y2="-9.25" width="0.127" layer="21"/>
<wire x1="3.25" y1="-9.25" x2="-3.25" y2="-9.25" width="0.127" layer="21"/>
<wire x1="-3.25" y1="-9.25" x2="-5.5" y2="-11.5" width="0.127" layer="21"/>
<wire x1="-5.5" y1="-11.5" x2="-7" y2="-11.5" width="0.127" layer="21"/>
<wire x1="-7" y1="-11.5" x2="-9.25" y2="-9.25" width="0.127" layer="21"/>
<wire x1="-9.25" y1="-9.25" x2="-16" y2="-9.25" width="0.127" layer="21"/>
<wire x1="-16" y1="-9.25" x2="-16" y2="9.25" width="0.127" layer="21"/>
<pad name="1" x="-6.25" y="8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="-6.25" y="-8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="6.25" y="8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="6.25" y="-8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-5.08" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B50">
<description>Becher B50 (cup B50)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 40x21x43
RM (grid) [mm]: 15x25
manufactured by NKL®</description>
<wire x1="-20" y1="10.5" x2="20" y2="10.5" width="0.127" layer="21"/>
<wire x1="20" y1="10.5" x2="20" y2="-10.5" width="0.127" layer="21"/>
<wire x1="20" y1="-10.5" x2="-20" y2="-10.5" width="0.127" layer="21"/>
<wire x1="-20" y1="-10.5" x2="-20" y2="10.5" width="0.127" layer="21"/>
<pad name="5" x="0" y="7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="6" x="0" y="-7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="1" x="12.5" y="7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="2" x="12.5" y="-7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="4" x="-12.5" y="-7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="3" x="-12.5" y="7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<text x="-8.89" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-19" y="0" drill="4"/>
<hole x="19" y="0" drill="4"/>
</package>
<package name="B40">
<description>Becher B40 (cup B40)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 35x20x36
RM (grid) [mm]: 12.5x20
manufactured by NKL®</description>
<wire x1="-17.5" y1="10" x2="17.5" y2="10" width="0.127" layer="21"/>
<wire x1="17.5" y1="10" x2="17.5" y2="-10" width="0.127" layer="21"/>
<wire x1="17.5" y1="-10" x2="-17.5" y2="-10" width="0.127" layer="21"/>
<wire x1="-17.5" y1="-10" x2="-17.5" y2="10" width="0.127" layer="21"/>
<pad name="5" x="0" y="6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="6" x="0" y="-6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="1" x="10" y="6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="2" x="10" y="-6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="4" x="-10" y="-6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="3" x="-10" y="6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<text x="-7.62" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-16" y="0" drill="4"/>
<hole x="16" y="0" drill="4"/>
</package>
<package name="KS1405">
<description>Kappe KS1405 (case KS1405)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 18x8x17
RM (grid) [mm]: 7.5(5)x5
manufactured by NKL®</description>
<wire x1="3.5" y1="5" x2="3.5" y2="-5" width="0.127" layer="21"/>
<wire x1="3.5" y1="-5" x2="-3.5" y2="-5" width="0.127" layer="21"/>
<wire x1="-3.5" y1="-5" x2="-3.5" y2="5" width="0.127" layer="21"/>
<wire x1="-3.5" y1="5" x2="3.5" y2="5" width="0.127" layer="21"/>
<wire x1="-4" y1="9" x2="4" y2="9" width="0.127" layer="21"/>
<wire x1="4" y1="9" x2="4" y2="-9" width="0.127" layer="21"/>
<wire x1="4" y1="-9" x2="-4" y2="-9" width="0.127" layer="21"/>
<wire x1="-4" y1="-9" x2="-4" y2="9" width="0.127" layer="21"/>
<pad name="2" x="2.5" y="-3.75" drill="0.8128" diameter="1.9304" shape="octagon"/>
<pad name="1" x="-2.5" y="-3.75" drill="0.8128" diameter="1.9304" shape="octagon"/>
<pad name="3" x="-2.5" y="3.75" drill="0.8128" diameter="1.9304" shape="octagon"/>
<pad name="4" x="2.5" y="3.75" drill="0.8128" diameter="1.9304" shape="octagon"/>
<pad name="5" x="-2.5" y="1.25" drill="0.8128" diameter="1.9304" shape="octagon"/>
<pad name="6" x="2.5" y="1.25" drill="0.8128" diameter="1.9304" shape="octagon"/>
<text x="-2.54" y="6.35" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-7.62" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="KS1908">
<description>Kappe KS1908 (case KS1908)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 26x16x26
RM (grid) [mm]: 12.5x10
manufactured by NKL®</description>
<wire x1="-6.75" y1="-10" x2="-6.75" y2="10" width="0.127" layer="21"/>
<wire x1="-6.75" y1="10" x2="6.75" y2="10" width="0.127" layer="21"/>
<wire x1="6.75" y1="10" x2="6.75" y2="-10" width="0.127" layer="21"/>
<wire x1="6.75" y1="-10" x2="-6.75" y2="-10" width="0.127" layer="21"/>
<wire x1="-8" y1="-13" x2="-8" y2="13" width="0.127" layer="21"/>
<wire x1="-8" y1="13" x2="8" y2="13" width="0.127" layer="21"/>
<wire x1="8" y1="13" x2="8" y2="-13" width="0.127" layer="21"/>
<wire x1="8" y1="-13" x2="-8" y2="-13" width="0.127" layer="21"/>
<pad name="2" x="5" y="-6.25" drill="1.016" diameter="2.54" shape="octagon"/>
<pad name="1" x="-5" y="-6.25" drill="1.016" diameter="2.54" shape="octagon"/>
<pad name="3" x="-5" y="6.25" drill="1.016" diameter="2.54" shape="octagon"/>
<pad name="4" x="5" y="6.25" drill="1.016" diameter="2.54" shape="octagon"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="KS2610">
<description>Kappe KS2610 (case KS2610)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 34x19x34
RM (grid) [mm]: 15x12.5
manufactured by NKL®</description>
<wire x1="-8.5" y1="-11" x2="-8.5" y2="11" width="0.127" layer="21"/>
<wire x1="-8.5" y1="11" x2="8.5" y2="11" width="0.127" layer="21"/>
<wire x1="8.5" y1="11" x2="8.5" y2="-11" width="0.127" layer="21"/>
<wire x1="8.5" y1="-11" x2="-8.5" y2="-11" width="0.127" layer="21"/>
<wire x1="-9.5" y1="-17" x2="-9.5" y2="17" width="0.127" layer="21"/>
<wire x1="-9.5" y1="17" x2="9.5" y2="17" width="0.127" layer="21"/>
<wire x1="9.5" y1="17" x2="9.5" y2="-17" width="0.127" layer="21"/>
<wire x1="9.5" y1="-17" x2="-9.5" y2="-17" width="0.127" layer="21"/>
<pad name="1" x="-6.25" y="-7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="-6.25" y="7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="6.25" y="7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="6.25" y="-7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="KS3213">
<description>Kappe KS3213 (case KS3213)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 40x20x38
RM (grid) [mm]: 17.5x15
manufactured by NKL®</description>
<wire x1="-9.5" y1="-12.5" x2="-9.5" y2="12.5" width="0.127" layer="21"/>
<wire x1="-9.5" y1="12.5" x2="9.5" y2="12.5" width="0.127" layer="21"/>
<wire x1="9.5" y1="12.5" x2="9.5" y2="-12.5" width="0.127" layer="21"/>
<wire x1="9.5" y1="-12.5" x2="-9.5" y2="-12.5" width="0.127" layer="21"/>
<wire x1="-10" y1="-20" x2="-10" y2="20" width="0.127" layer="21"/>
<wire x1="-10" y1="20" x2="10" y2="20" width="0.127" layer="21"/>
<wire x1="10" y1="20" x2="10" y2="-20" width="0.127" layer="21"/>
<wire x1="10" y1="-20" x2="-10" y2="-20" width="0.127" layer="21"/>
<pad name="1" x="-7.5" y="-8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="-7.5" y="8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="7.5" y="8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="7.5" y="-8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="11-20">
<description>R2006 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 10mm
(ØxB(W))[mm]: 25x10
manufactured by NKL®</description>
<wire x1="-4" y1="12" x2="-4" y2="-12" width="0.127" layer="21"/>
<wire x1="-4" y1="-12" x2="4" y2="-12" width="0.127" layer="21"/>
<wire x1="4" y1="-12" x2="4" y2="12" width="0.127" layer="21"/>
<wire x1="4" y1="12" x2="-4" y2="12" width="0.127" layer="21"/>
<wire x1="-5" y1="0" x2="-4" y2="0" width="0.6096" layer="51"/>
<wire x1="4" y1="0" x2="5" y2="0" width="0.6096" layer="51"/>
<wire x1="-5" y1="12" x2="5" y2="12" width="0.6096" layer="21"/>
<wire x1="-5" y1="11" x2="5" y2="11" width="0.6096" layer="21"/>
<wire x1="-5" y1="10" x2="5" y2="10" width="0.6096" layer="21"/>
<wire x1="-5" y1="9" x2="5" y2="9" width="0.6096" layer="21"/>
<wire x1="-5" y1="8" x2="5" y2="8" width="0.6096" layer="21"/>
<wire x1="-5" y1="7" x2="5" y2="7" width="0.6096" layer="21"/>
<wire x1="-5" y1="4" x2="5" y2="4" width="0.6096" layer="21"/>
<wire x1="-5" y1="3" x2="5" y2="3" width="0.6096" layer="21"/>
<wire x1="-5" y1="2" x2="5" y2="2" width="0.6096" layer="21"/>
<wire x1="-5" y1="-2" x2="5" y2="-2" width="0.6096" layer="21"/>
<wire x1="-5" y1="-3" x2="5" y2="-3" width="0.6096" layer="21"/>
<wire x1="-5" y1="-4" x2="5" y2="-4" width="0.6096" layer="21"/>
<wire x1="-5" y1="-7" x2="5" y2="-7" width="0.6096" layer="21"/>
<wire x1="-5" y1="-8" x2="5" y2="-8" width="0.6096" layer="21"/>
<wire x1="-5" y1="-9" x2="5" y2="-9" width="0.6096" layer="21"/>
<wire x1="-5" y1="-10" x2="5" y2="-10" width="0.6096" layer="21"/>
<wire x1="-5" y1="-11" x2="5" y2="-11" width="0.6096" layer="21"/>
<wire x1="-5" y1="-12" x2="5" y2="-12" width="0.6096" layer="21"/>
<wire x1="-4" y1="0" x2="4" y2="0" width="0.6096" layer="27"/>
<pad name="1" x="-5" y="0" drill="0.8128" shape="long" rot="R90"/>
<pad name="2" x="5" y="0" drill="0.8128" shape="long" rot="R90"/>
<text x="-6.35" y="1.27" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="7.62" y="1.27" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="11-17">
<description>R1705 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 8mm
(ØxB(W))[mm]: 21x8
manufactured by NKL®</description>
<wire x1="-3" y1="9" x2="3" y2="9" width="0.127" layer="21"/>
<wire x1="3" y1="9" x2="3" y2="0" width="0.127" layer="21"/>
<wire x1="3" y1="0" x2="3" y2="-9" width="0.127" layer="21"/>
<wire x1="3" y1="-9" x2="-3" y2="-9" width="0.127" layer="21"/>
<wire x1="-3" y1="-9" x2="-3" y2="0" width="0.127" layer="21"/>
<wire x1="-3" y1="0" x2="-3" y2="9" width="0.127" layer="21"/>
<wire x1="-3" y1="0" x2="3" y2="0" width="0.4064" layer="21"/>
<wire x1="-4" y1="1" x2="4" y2="1" width="0.4064" layer="21"/>
<wire x1="-4" y1="-1" x2="4" y2="-1" width="0.4064" layer="21"/>
<wire x1="-4" y1="-2" x2="4" y2="-2" width="0.4064" layer="21"/>
<wire x1="-4" y1="2" x2="4" y2="2" width="0.4064" layer="21"/>
<wire x1="-4" y1="4" x2="4" y2="4" width="0.4064" layer="21"/>
<wire x1="-4" y1="5" x2="4" y2="5" width="0.4064" layer="21"/>
<wire x1="-4" y1="6" x2="4" y2="6" width="0.4064" layer="21"/>
<wire x1="-4" y1="7" x2="4" y2="7" width="0.4064" layer="21"/>
<wire x1="-4" y1="8" x2="4" y2="8" width="0.4064" layer="21"/>
<wire x1="-4" y1="9" x2="4" y2="9" width="0.4064" layer="21"/>
<wire x1="-4" y1="-4" x2="4" y2="-4" width="0.4064" layer="21"/>
<wire x1="-4" y1="-5" x2="4" y2="-5" width="0.4064" layer="21"/>
<wire x1="-4" y1="-6" x2="4" y2="-6" width="0.4064" layer="21"/>
<wire x1="-4" y1="-7" x2="4" y2="-7" width="0.4064" layer="21"/>
<wire x1="-4" y1="-8" x2="4" y2="-8" width="0.4064" layer="21"/>
<wire x1="-4" y1="-9" x2="4" y2="-9" width="0.4064" layer="21"/>
<wire x1="-4" y1="0" x2="-3" y2="0" width="0.4064" layer="51"/>
<wire x1="3" y1="0" x2="4" y2="0" width="0.4064" layer="51"/>
<pad name="1" x="-4" y="0" drill="0.8128" shape="long" rot="R90"/>
<pad name="2" x="4" y="0" drill="0.8128" shape="long" rot="R90"/>
<text x="-5.08" y="0" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="6.35" y="0" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="10-17">
<description>R1705 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 8mm
(ØxH)[mm]: 21x8
manufactured by NKL®</description>
<wire x1="0" y1="4" x2="0" y2="10" width="0.6096" layer="21"/>
<wire x1="4" y1="0" x2="10" y2="0" width="0.6096" layer="21"/>
<wire x1="0" y1="-4" x2="0" y2="-10" width="0.6096" layer="21"/>
<wire x1="1.5" y1="-4" x2="3" y2="-9.5" width="0.6096" layer="21"/>
<wire x1="1.5" y1="4" x2="3" y2="9.5" width="0.6096" layer="21"/>
<wire x1="2.5" y1="3.5" x2="6" y2="8" width="0.6096" layer="21"/>
<wire x1="2.5" y1="-3.5" x2="6" y2="-8" width="0.6096" layer="21"/>
<wire x1="3.5" y1="2.5" x2="8" y2="6" width="0.6096" layer="21"/>
<wire x1="3.5" y1="-2.5" x2="8" y2="-6" width="0.6096" layer="21"/>
<wire x1="4" y1="-1" x2="9.5" y2="-3.5" width="0.6096" layer="21"/>
<wire x1="4" y1="1" x2="9.5" y2="3.5" width="0.6096" layer="21"/>
<wire x1="-10" y1="0" x2="-4" y2="0" width="0.6096" layer="21"/>
<wire x1="-4" y1="1" x2="-9.5" y2="3.5" width="0.6096" layer="21"/>
<wire x1="-4" y1="-1" x2="-9.5" y2="-3.5" width="0.6096" layer="21"/>
<wire x1="-3.5" y1="2.5" x2="-8" y2="6" width="0.6096" layer="21"/>
<wire x1="-3.5" y1="-2.5" x2="-8" y2="-6" width="0.6096" layer="21"/>
<wire x1="-1.5" y1="4" x2="-3" y2="9.5" width="0.6096" layer="21"/>
<wire x1="-1.5" y1="-4" x2="-3" y2="-9.5" width="0.6096" layer="21"/>
<wire x1="-2.5" y1="3.5" x2="-6" y2="8" width="0.6096" layer="21"/>
<wire x1="-2.5" y1="-3.5" x2="-6" y2="-8" width="0.6096" layer="21"/>
<wire x1="-11" y1="0" x2="-10" y2="0" width="0.6096" layer="51"/>
<wire x1="-3" y1="0" x2="-4.5" y2="0.5" width="0.6096" layer="51"/>
<circle x="0" y="0" radius="9" width="0.127" layer="21"/>
<circle x="0" y="0" radius="5" width="0.127" layer="21"/>
<pad name="2" x="-3" y="0" drill="0.8128" shape="long" rot="R90"/>
<pad name="1" x="-11" y="0" drill="0.8128" shape="long" rot="R90"/>
<text x="-2.54" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="10-20">
<description>R2006 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 9mm
(ØxH)[mm]: 25x12
manufactured by NKL®</description>
<wire x1="5" y1="0" x2="11" y2="0" width="0.6096" layer="21"/>
<wire x1="-5" y1="0" x2="-11" y2="0" width="0.6096" layer="21"/>
<wire x1="0" y1="5" x2="0" y2="11" width="0.6096" layer="21"/>
<wire x1="0" y1="-5" x2="0" y2="-11" width="0.6096" layer="21"/>
<wire x1="-4" y1="-3" x2="-9" y2="-6" width="0.6096" layer="21"/>
<wire x1="4" y1="-3" x2="9" y2="-6.5" width="0.6096" layer="21"/>
<wire x1="4" y1="3" x2="9" y2="7" width="0.6096" layer="21"/>
<wire x1="-4" y1="3" x2="-9" y2="7" width="0.6096" layer="21"/>
<wire x1="1" y1="-5" x2="2" y2="-11" width="0.6096" layer="21"/>
<wire x1="-2" y1="-11" x2="-1" y2="-5" width="0.6096" layer="21"/>
<wire x1="-5" y1="-1" x2="-11" y2="-2" width="0.6096" layer="21"/>
<wire x1="-5" y1="1" x2="-11" y2="2" width="0.6096" layer="21"/>
<wire x1="-1" y1="5" x2="-2" y2="11" width="0.6096" layer="21"/>
<wire x1="1" y1="5" x2="2" y2="11" width="0.6096" layer="21"/>
<wire x1="5" y1="1" x2="11" y2="2" width="0.6096" layer="21"/>
<wire x1="5" y1="-1" x2="11" y2="-2" width="0.6096" layer="21"/>
<wire x1="2" y1="4.5" x2="4" y2="10.5" width="0.6096" layer="21"/>
<wire x1="-2" y1="4.5" x2="-4" y2="10.5" width="0.6096" layer="21"/>
<wire x1="-2" y1="-4.5" x2="-4" y2="-10.5" width="0.6096" layer="21"/>
<wire x1="2" y1="-4.5" x2="4" y2="-10.5" width="0.6096" layer="21"/>
<wire x1="-3" y1="-4" x2="-6.5" y2="-9" width="0.6096" layer="21"/>
<wire x1="3" y1="-4" x2="6.5" y2="-9" width="0.6096" layer="21"/>
<wire x1="-4.5" y1="-2" x2="-10.5" y2="-4" width="0.6096" layer="21"/>
<wire x1="-4.5" y1="2" x2="-10.5" y2="4" width="0.6096" layer="21"/>
<wire x1="4.5" y1="2" x2="10.5" y2="4" width="0.6096" layer="21"/>
<wire x1="4.5" y1="-2" x2="10.5" y2="-4" width="0.6096" layer="21"/>
<wire x1="3" y1="4" x2="6" y2="9.5" width="0.6096" layer="21"/>
<wire x1="-3" y1="4" x2="-6" y2="9.5" width="0.6096" layer="21"/>
<wire x1="-12" y1="0" x2="-11" y2="0" width="0.6096" layer="51"/>
<wire x1="-5.5" y1="0.5" x2="-3" y2="0" width="0.6096" layer="51"/>
<circle x="0" y="0" radius="10" width="0.127" layer="21"/>
<circle x="0" y="0" radius="6" width="0.127" layer="21"/>
<pad name="2" x="-3" y="0" drill="0.8128" shape="long" rot="R90"/>
<pad name="1" x="-12" y="0" drill="0.8128" shape="long" rot="R90"/>
<text x="-2.54" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="11-13">
<description>R1305 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 8mm
(ØxB(W))[mm]: 16x8
manufactured by NKL®</description>
<wire x1="-3" y1="7" x2="-3" y2="0" width="0.127" layer="21"/>
<wire x1="-3" y1="0" x2="-3" y2="-7" width="0.127" layer="21"/>
<wire x1="-3" y1="-7" x2="3" y2="-7" width="0.127" layer="21"/>
<wire x1="3" y1="-7" x2="3" y2="0" width="0.127" layer="21"/>
<wire x1="3" y1="0" x2="3" y2="7" width="0.127" layer="21"/>
<wire x1="3" y1="7" x2="-3" y2="7" width="0.127" layer="21"/>
<wire x1="-3" y1="0" x2="3" y2="0" width="0.4064" layer="21"/>
<wire x1="-4" y1="1.5" x2="4" y2="1.5" width="0.4064" layer="21"/>
<wire x1="-4" y1="4.5" x2="4" y2="4.5" width="0.4064" layer="21"/>
<wire x1="-4" y1="6" x2="4" y2="6" width="0.4064" layer="21"/>
<wire x1="-4" y1="7" x2="4" y2="7" width="0.4064" layer="21"/>
<wire x1="-4" y1="-1.5" x2="4" y2="-1.5" width="0.4064" layer="21"/>
<wire x1="-4" y1="-4.5" x2="4" y2="-4.5" width="0.4064" layer="21"/>
<wire x1="-4" y1="-6" x2="4" y2="-6" width="0.4064" layer="21"/>
<wire x1="-4" y1="-7" x2="4" y2="-7" width="0.4064" layer="21"/>
<wire x1="-4" y1="0" x2="-3" y2="0" width="0.4064" layer="51"/>
<wire x1="3" y1="0" x2="4" y2="0" width="0.4064" layer="51"/>
<pad name="1" x="-4" y="0" drill="0.8128" shape="long" rot="R90"/>
<pad name="2" x="4" y="0" drill="0.8128" shape="long" rot="R90"/>
<text x="-5.08" y="-2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="6.35" y="-2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="KS1303">
<description>Kappe KS1303 (case KS1303)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 16x8x17
RM (grid) [mm]: 7.5(5)x5
manufactured by NKL®</description>
<wire x1="3.5" y1="-5.5" x2="3.5" y2="5.5" width="0.127" layer="21"/>
<wire x1="3.5" y1="5.5" x2="-3.5" y2="5.5" width="0.127" layer="21"/>
<wire x1="-3.5" y1="5.5" x2="-3.5" y2="-5.5" width="0.127" layer="21"/>
<wire x1="-3.5" y1="-5.5" x2="3.5" y2="-5.5" width="0.127" layer="21"/>
<wire x1="-4" y1="8" x2="-4" y2="-8" width="0.127" layer="21"/>
<wire x1="-4" y1="-8" x2="4" y2="-8" width="0.127" layer="21"/>
<wire x1="4" y1="-8" x2="4" y2="8" width="0.127" layer="21"/>
<wire x1="4" y1="8" x2="-4" y2="8" width="0.127" layer="21"/>
<pad name="2" x="2.5" y="-3.75" drill="0.6096" diameter="1.6764" shape="octagon"/>
<pad name="1" x="-2.5" y="-3.75" drill="0.6096" diameter="1.6764" shape="octagon"/>
<pad name="4" x="2.5" y="3.75" drill="0.6096" diameter="1.6764" shape="octagon"/>
<pad name="3" x="-2.5" y="3.75" drill="0.6096" diameter="1.6764" shape="octagon"/>
<pad name="5" x="-2.5" y="1.25" drill="0.6096" diameter="1.6764" shape="octagon"/>
<pad name="6" x="2.5" y="1.25" drill="0.6096" diameter="1.6764" shape="octagon"/>
<text x="-2.54" y="6.35" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-7.62" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="KS1003">
<description>Kappe KS1003 (case KS1003)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 13x6x13
RM (grid) [mm]: 7.5(5)x4
manufactured by NKL®</description>
<wire x1="-3" y1="5" x2="-3" y2="-5" width="0.127" layer="25"/>
<wire x1="-3" y1="-5" x2="3" y2="-5" width="0.127" layer="21"/>
<wire x1="3" y1="-5" x2="3" y2="5" width="0.127" layer="25"/>
<wire x1="3" y1="5" x2="-3" y2="5" width="0.127" layer="21"/>
<wire x1="-3" y1="6.5" x2="-3" y2="-5" width="0.127" layer="21"/>
<wire x1="-3" y1="-5" x2="-3" y2="-6.5" width="0.127" layer="21"/>
<wire x1="-3" y1="-6.5" x2="3" y2="-6.5" width="0.127" layer="21"/>
<wire x1="3" y1="-6.5" x2="3" y2="-5" width="0.127" layer="21"/>
<wire x1="3" y1="-5" x2="3" y2="6.5" width="0.127" layer="21"/>
<wire x1="3" y1="6.5" x2="-3" y2="6.5" width="0.127" layer="21"/>
<pad name="3" x="-2" y="3.75" drill="0.4064" diameter="1.4224" shape="octagon"/>
<pad name="2" x="2" y="-3.75" drill="0.4064" diameter="1.4224" shape="octagon"/>
<pad name="4" x="2" y="3.75" drill="0.4064" diameter="1.4224" shape="octagon"/>
<pad name="1" x="-2" y="-3.75" drill="0.4064" diameter="1.4224" shape="octagon"/>
<pad name="5" x="-2" y="1.25" drill="0.4064" diameter="1.4224" shape="octagon"/>
<pad name="6" x="2" y="1.25" drill="0.4064" diameter="1.4224" shape="octagon"/>
<text x="-3.81" y="-3.81" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="1.27" y="-2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="11-14">
<description>R1405 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 6x8mm
(ØxB(W))[mm]: 16x8
manufactured by NKL®</description>
<wire x1="-3" y1="-3.5" x2="-3" y2="-7" width="0.127" layer="21"/>
<wire x1="-3" y1="-7" x2="3" y2="-7" width="0.127" layer="21"/>
<wire x1="3" y1="-7" x2="3" y2="-3.5" width="0.127" layer="21"/>
<wire x1="-3" y1="3.5" x2="-3" y2="7" width="0.127" layer="21"/>
<wire x1="-3" y1="7" x2="3" y2="7" width="0.127" layer="21"/>
<wire x1="3" y1="7" x2="3" y2="3.5" width="0.127" layer="21"/>
<wire x1="3" y1="2.5" x2="3" y2="-2.5" width="0.127" layer="21"/>
<wire x1="-3" y1="-2.5" x2="-3" y2="2.5" width="0.127" layer="21"/>
<wire x1="-4" y1="1" x2="4" y2="1" width="0.4064" layer="21"/>
<wire x1="-4" y1="-1" x2="4" y2="-1" width="0.4064" layer="21"/>
<wire x1="-2.5" y1="-3" x2="2.5" y2="-3" width="0.4064" layer="21"/>
<wire x1="-4" y1="-2" x2="4" y2="-2" width="0.4064" layer="21"/>
<wire x1="-4" y1="-4" x2="4" y2="-4" width="0.4064" layer="21"/>
<wire x1="-4" y1="-4.73" x2="4" y2="-4.73" width="0.4064" layer="21"/>
<wire x1="-4" y1="-7" x2="4" y2="-7" width="0.4064" layer="21"/>
<wire x1="-4" y1="2" x2="4" y2="2" width="0.4064" layer="21"/>
<wire x1="-4" y1="4" x2="4" y2="4" width="0.4064" layer="21"/>
<wire x1="-4" y1="4.73" x2="4" y2="4.73" width="0.4064" layer="21"/>
<wire x1="-4" y1="7" x2="4" y2="7" width="0.4064" layer="21"/>
<wire x1="-2.5" y1="3" x2="2.5" y2="3" width="0.4064" layer="21"/>
<wire x1="-4" y1="3" x2="-2.5" y2="3" width="0.4064" layer="51"/>
<wire x1="2.5" y1="3" x2="4" y2="3" width="0.4064" layer="51"/>
<wire x1="2.5" y1="-3" x2="4" y2="-3" width="0.4064" layer="51"/>
<wire x1="-4" y1="-3" x2="-2" y2="-3" width="0.4064" layer="51"/>
<pad name="3" x="-4" y="3" drill="0.8128" shape="long"/>
<pad name="2" x="4" y="-3" drill="0.8128" shape="long"/>
<pad name="1" x="-4" y="-3" drill="0.8128" shape="long"/>
<pad name="4" x="4" y="3" drill="0.8128" shape="long"/>
<text x="-6.35" y="-2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="7.62" y="-2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="-4.5" y1="-0.5" x2="4.5" y2="0.5" layer="21"/>
</package>
<package name="11-19">
<description>R1908 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 8x12mm
(ØxB(W))[mm]: 24x12
manufactured by NKL®</description>
<wire x1="-6" y1="5" x2="-6" y2="6" width="0.127" layer="21"/>
<wire x1="-6" y1="6" x2="-6" y2="10" width="0.127" layer="21"/>
<wire x1="-6" y1="10" x2="-6" y2="12" width="0.127" layer="21"/>
<wire x1="6" y1="12" x2="6" y2="10" width="0.127" layer="21"/>
<wire x1="6" y1="10" x2="6" y2="6" width="0.127" layer="21"/>
<wire x1="6" y1="6" x2="6" y2="5" width="0.127" layer="21"/>
<wire x1="6" y1="-5" x2="6" y2="-8" width="0.127" layer="21"/>
<wire x1="6" y1="-8" x2="6" y2="-10" width="0.127" layer="21"/>
<wire x1="6" y1="-10" x2="6" y2="-12" width="0.127" layer="21"/>
<wire x1="-6" y1="-12" x2="-6" y2="-10" width="0.127" layer="21"/>
<wire x1="-6" y1="-10" x2="-6" y2="-8" width="0.127" layer="21"/>
<wire x1="-6" y1="-8" x2="-6" y2="-5" width="0.127" layer="21"/>
<wire x1="-6" y1="-3" x2="-6" y2="-2" width="0.127" layer="21"/>
<wire x1="-6" y1="-2" x2="-6" y2="2" width="0.127" layer="21"/>
<wire x1="-6" y1="2" x2="-6" y2="3" width="0.127" layer="21"/>
<wire x1="6" y1="3" x2="6" y2="2" width="0.127" layer="21"/>
<wire x1="6" y1="2" x2="6" y2="-2" width="0.127" layer="21"/>
<wire x1="6" y1="-2" x2="6" y2="-3" width="0.127" layer="21"/>
<wire x1="-6" y1="2" x2="6" y2="2" width="0.6096" layer="21"/>
<wire x1="-6" y1="-2" x2="6" y2="-2" width="0.6096" layer="21"/>
<wire x1="6" y1="-8" x2="-6" y2="-8" width="0.6096" layer="21"/>
<wire x1="-6" y1="-10" x2="6" y2="-10" width="0.6096" layer="21"/>
<wire x1="6" y1="-12" x2="-6" y2="-12" width="0.6096" layer="21"/>
<wire x1="-6" y1="6" x2="6" y2="6" width="0.6096" layer="21"/>
<wire x1="-6" y1="10" x2="6" y2="10" width="0.6096" layer="21"/>
<wire x1="-6" y1="12" x2="6" y2="12" width="0.6096" layer="21"/>
<wire x1="-6" y1="4" x2="-4" y2="4" width="0.6096" layer="51"/>
<wire x1="4" y1="4" x2="6" y2="4" width="0.6096" layer="51"/>
<wire x1="6" y1="-4" x2="4" y2="-4" width="0.6096" layer="51"/>
<wire x1="-6" y1="-4" x2="-4" y2="-4" width="0.6096" layer="51"/>
<wire x1="-4.5" y1="4" x2="4.5" y2="4" width="0.6096" layer="21"/>
<wire x1="-4.5" y1="-4" x2="4.5" y2="-4" width="0.6096" layer="21"/>
<pad name="3" x="-6" y="4" drill="0.8128" shape="long"/>
<pad name="2" x="6" y="-4" drill="0.8128" shape="long"/>
<pad name="1" x="-6" y="-4" drill="0.8128" shape="long"/>
<pad name="4" x="6" y="4" drill="0.8128" shape="long"/>
<text x="-7.62" y="-2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="8.89" y="-2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="-6.5" y1="-0.5" x2="6.5" y2="0.5" layer="21"/>
</package>
<package name="B10">
<description>Becher B10 (cup B10)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 18x10x21
RM (grid) [mm]: 5x10
manufactured by NKL®</description>
<wire x1="-9" y1="5" x2="9" y2="5" width="0.127" layer="21"/>
<wire x1="9" y1="5" x2="9" y2="-5" width="0.127" layer="21"/>
<wire x1="9" y1="-5" x2="-9" y2="-5" width="0.127" layer="21"/>
<wire x1="-9" y1="-5" x2="-9" y2="5" width="0.127" layer="21"/>
<pad name="5" x="0" y="2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="6" x="0" y="-2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="1" x="5" y="2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="2" x="5" y="-2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="4" x="-5" y="-2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="3" x="-5" y="2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<text x="-7.62" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-1.27" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-8" y="0" drill="3"/>
<hole x="8" y="0" drill="3"/>
</package>
<package name="B30">
<description>Becher B30 (cup B30)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 27x14x30
RM (grid) [mm]: 7.5x15
manufactured by NKL®</description>
<wire x1="-13.5" y1="7" x2="13.5" y2="7" width="0.127" layer="21"/>
<wire x1="13.5" y1="7" x2="13.5" y2="-7" width="0.127" layer="21"/>
<wire x1="13.5" y1="-7" x2="-13.5" y2="-7" width="0.127" layer="21"/>
<wire x1="-13.5" y1="-7" x2="-13.5" y2="7" width="0.127" layer="21"/>
<pad name="5" x="0" y="3.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="6" x="0" y="-3.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="1" x="7.5" y="3.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="7.5" y="-3.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="-7.5" y="-3.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="-7.5" y="3.75" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-10.16" y="7.62" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-1.27" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-12.5" y="0" drill="4"/>
<hole x="12.5" y="0" drill="4"/>
</package>
<package name="B34">
<description>Becher B34 (cup B34)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 34x21(27/33)
RM (grid) [mm]: 12.5 / 25 / 22.5x15
manufactured by NKL®</description>
<circle x="0" y="0" radius="17" width="0.127" layer="21"/>
<pad name="6" x="-12.5" y="0" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="8" x="12.5" y="0" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="5" x="-6.25" y="0" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="7" x="6.25" y="0" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="1" x="-11.25" y="7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="11.25" y="7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="11.25" y="-7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="-11.25" y="-7.5" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="8.89" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-8.89" size="1.27" layer="27">&gt;VALUE</text>
<hole x="0" y="0" drill="3.81"/>
</package>
<package name="B5Ø">
<description>Becher B50 rund (cup B50 round)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 50x33
RM (grid) [mm]: 20/40x10 / 30x30
manufactured by NKL®</description>
<circle x="0" y="0" radius="25" width="0.127" layer="21"/>
<pad name="10" x="-5" y="10" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="9" x="5" y="10" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="11" x="5" y="-5" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="12" x="-5" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="5" x="5" y="20" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="6" x="-5" y="20" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="8" x="-5" y="-20" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="7" x="5" y="-20" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="4" x="-15" y="-15" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="15" y="-15" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="1" x="15" y="15" drill="1.4224" diameter="3.81" shape="octagon"/>
<pad name="2" x="-15" y="15" drill="1.4224" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-1.27" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B44">
<description>Becher B44 (cup B44)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 44x25(38)
RM (grid) [mm]: 2*7.3 / 17.2
manufactured by NKL®</description>
<circle x="0" y="0" radius="22" width="0.127" layer="21"/>
<pad name="1" x="-7.3" y="0" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="7.3" y="0" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="17.3" y="0" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-2.54" y="7.62" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-7.62" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="11-24">
<description>R2408 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 10mm
(ØxB(W))[mm]: 28x12
manufactured by NKL®</description>
<wire x1="4" y1="12" x2="4" y2="-12" width="0.127" layer="51"/>
<wire x1="-4" y1="-12" x2="-4" y2="12" width="0.127" layer="51"/>
<wire x1="-5" y1="1" x2="5" y2="1" width="0.6096" layer="21"/>
<wire x1="-5" y1="-1" x2="5" y2="-1" width="0.6096" layer="21"/>
<wire x1="-5" y1="-2" x2="5" y2="-2" width="0.6096" layer="21"/>
<wire x1="-5" y1="-3" x2="5" y2="-3" width="0.6096" layer="21"/>
<wire x1="-5" y1="-4" x2="5" y2="-4" width="0.6096" layer="21"/>
<wire x1="-5" y1="-5" x2="5" y2="-5" width="0.6096" layer="21"/>
<wire x1="-5" y1="-8" x2="5" y2="-8" width="0.6096" layer="21"/>
<wire x1="-5" y1="-9" x2="5" y2="-9" width="0.6096" layer="21"/>
<wire x1="-5" y1="-10" x2="5" y2="-10" width="0.6096" layer="21"/>
<wire x1="-5" y1="-11" x2="5" y2="-11" width="0.6096" layer="21"/>
<wire x1="-5" y1="-12" x2="-4" y2="-12" width="0.6096" layer="21"/>
<wire x1="-4" y1="-12" x2="4" y2="-12" width="0.6096" layer="21"/>
<wire x1="4" y1="-12" x2="5" y2="-12" width="0.6096" layer="21"/>
<wire x1="-5" y1="2" x2="5" y2="2" width="0.6096" layer="21"/>
<wire x1="-5" y1="3" x2="5" y2="3" width="0.6096" layer="21"/>
<wire x1="-5" y1="4" x2="5" y2="4" width="0.6096" layer="21"/>
<wire x1="-5" y1="5" x2="5" y2="5" width="0.6096" layer="21"/>
<wire x1="-5" y1="8" x2="5" y2="8" width="0.6096" layer="21"/>
<wire x1="-5" y1="9" x2="5" y2="9" width="0.6096" layer="21"/>
<wire x1="-5" y1="10" x2="5" y2="10" width="0.6096" layer="21"/>
<wire x1="-5" y1="11" x2="5" y2="11" width="0.6096" layer="21"/>
<wire x1="-5" y1="12" x2="-4" y2="12" width="0.6096" layer="21"/>
<wire x1="-4" y1="12" x2="4" y2="12" width="0.6096" layer="21"/>
<wire x1="4" y1="12" x2="5" y2="12" width="0.6096" layer="21"/>
<wire x1="-5" y1="7" x2="-4" y2="7" width="0.6096" layer="27"/>
<wire x1="-5" y1="6" x2="-4" y2="6" width="0.6096" layer="27"/>
<wire x1="4" y1="7" x2="5" y2="7" width="0.6096" layer="27"/>
<wire x1="4" y1="6" x2="5" y2="6" width="0.6096" layer="27"/>
<wire x1="4" y1="-6" x2="5" y2="-6" width="0.6096" layer="27"/>
<wire x1="4" y1="-7" x2="5" y2="-7" width="0.6096" layer="27"/>
<wire x1="-5" y1="-7" x2="-4" y2="-7" width="0.6096" layer="27"/>
<wire x1="-5" y1="-6" x2="-4" y2="-6" width="0.6096" layer="27"/>
<wire x1="-4" y1="-12" x2="-4" y2="-0.7" width="0.127" layer="21"/>
<wire x1="4" y1="12" x2="4" y2="0.7" width="0.127" layer="21"/>
<wire x1="-4" y1="0.7" x2="-4" y2="12" width="0.127" layer="21"/>
<wire x1="4" y1="-0.7" x2="4" y2="-12" width="0.127" layer="21"/>
<pad name="1" x="-5" y="0" drill="0.8128" shape="long"/>
<pad name="2" x="5" y="0" drill="0.8128" shape="long"/>
<text x="-6.35" y="1.27" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="7.62" y="1.27" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="11-26">
<description>R2610 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 12mm
(ØxB(W))[mm]: 31x15
manufactured by NKL®</description>
<wire x1="-5" y1="13" x2="5" y2="13" width="0.127" layer="21"/>
<wire x1="5" y1="13" x2="5" y2="-13" width="0.127" layer="21"/>
<wire x1="5" y1="-13" x2="-5" y2="-13" width="0.127" layer="21"/>
<wire x1="-5" y1="-13" x2="-5" y2="13" width="0.127" layer="21"/>
<wire x1="-7" y1="0" x2="7" y2="0" width="0.6096" layer="21"/>
<wire x1="-7" y1="-2" x2="7" y2="-2" width="0.6096" layer="21"/>
<wire x1="-7" y1="-6" x2="7" y2="-6" width="0.6096" layer="21"/>
<wire x1="-7" y1="-8" x2="7" y2="-8" width="0.6096" layer="21"/>
<wire x1="-7" y1="-10" x2="7" y2="-10" width="0.6096" layer="21"/>
<wire x1="-7" y1="-11" x2="7" y2="-11" width="0.6096" layer="21"/>
<wire x1="-7" y1="-12" x2="7" y2="-12" width="0.6096" layer="21"/>
<wire x1="-7" y1="-13" x2="7" y2="-13" width="0.6096" layer="21"/>
<wire x1="-7" y1="2" x2="7" y2="2" width="0.6096" layer="21"/>
<wire x1="-7" y1="6" x2="7" y2="6" width="0.6096" layer="21"/>
<wire x1="-7" y1="8" x2="7" y2="8" width="0.6096" layer="21"/>
<wire x1="-7" y1="10" x2="7" y2="10" width="0.6096" layer="21"/>
<wire x1="-7" y1="11" x2="7" y2="11" width="0.6096" layer="21"/>
<wire x1="-7" y1="12" x2="7" y2="12" width="0.6096" layer="21"/>
<wire x1="-7" y1="13" x2="7" y2="13" width="0.6096" layer="21"/>
<wire x1="-7" y1="4" x2="-4" y2="4" width="0.6096" layer="51"/>
<wire x1="3" y1="4" x2="7" y2="4" width="0.6096" layer="51"/>
<wire x1="3" y1="-4" x2="7" y2="-4" width="0.6096" layer="51"/>
<wire x1="-7" y1="-4" x2="-4" y2="-4" width="0.6096" layer="51"/>
<pad name="1" x="-7" y="4" drill="0.8128" shape="long"/>
<pad name="2" x="7" y="4" drill="0.8128" shape="long"/>
<pad name="3" x="-7" y="-4" drill="0.8128" shape="long"/>
<pad name="4" x="7" y="-4" drill="0.8128" shape="long"/>
<text x="-8.89" y="-2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="10.16" y="-2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="11-27">
<description>R2711 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 16mm
(ØxB(W))[mm]: 32x18
manufactured by NKL®</description>
<wire x1="-6" y1="14" x2="6" y2="14" width="0.127" layer="21"/>
<wire x1="6" y1="14" x2="6" y2="0" width="0.127" layer="21"/>
<wire x1="6" y1="0" x2="6" y2="-14" width="0.127" layer="21"/>
<wire x1="6" y1="-14" x2="-6" y2="-14" width="0.127" layer="21"/>
<wire x1="-6" y1="-14" x2="-6" y2="0" width="0.127" layer="21"/>
<wire x1="-6" y1="0" x2="-6" y2="14" width="0.127" layer="21"/>
<wire x1="-8" y1="2" x2="8" y2="2" width="0.6096" layer="21"/>
<wire x1="-8" y1="4" x2="8" y2="4" width="0.6096" layer="21"/>
<wire x1="-8" y1="9" x2="8" y2="9" width="0.6096" layer="21"/>
<wire x1="-8" y1="11" x2="8" y2="11" width="0.6096" layer="21"/>
<wire x1="-8" y1="12" x2="8" y2="12" width="0.6096" layer="21"/>
<wire x1="-8" y1="13" x2="8" y2="13" width="0.6096" layer="21"/>
<wire x1="-8" y1="14" x2="8" y2="14" width="0.6096" layer="21"/>
<wire x1="-8" y1="6" x2="8" y2="6" width="0.6096" layer="21"/>
<wire x1="-8" y1="-2" x2="8" y2="-2" width="0.6096" layer="21"/>
<wire x1="-8" y1="-4" x2="8" y2="-4" width="0.6096" layer="21"/>
<wire x1="-8" y1="-6" x2="8" y2="-6" width="0.6096" layer="21"/>
<wire x1="-8" y1="-9" x2="8" y2="-9" width="0.6096" layer="21"/>
<wire x1="-8" y1="-11" x2="8" y2="-11" width="0.6096" layer="21"/>
<wire x1="-8" y1="-12" x2="8" y2="-12" width="0.6096" layer="21"/>
<wire x1="-8" y1="-13" x2="8" y2="-13" width="0.6096" layer="21"/>
<wire x1="-8" y1="-14" x2="8" y2="-14" width="0.6096" layer="21"/>
<wire x1="-6" y1="0" x2="6" y2="0" width="0.6096" layer="21"/>
<wire x1="-8" y1="0" x2="-6" y2="0" width="0.6096" layer="51"/>
<wire x1="6" y1="0" x2="8" y2="0" width="0.6096" layer="51"/>
<wire x1="-8" y1="15" x2="8" y2="15" width="0.6096" layer="21"/>
<wire x1="-8" y1="-15" x2="8" y2="-15" width="0.6096" layer="21"/>
<pad name="1" x="-8" y="0" drill="0.8128" shape="long"/>
<pad name="2" x="8" y="0" drill="0.8128" shape="long"/>
<text x="-8.89" y="2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="10.16" y="2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="11-32">
<description>R3213 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 18mm
(ØxB(W))[mm]: 36x18
manufactured by NKL®</description>
<wire x1="-7" y1="16" x2="7" y2="16" width="0.127" layer="21"/>
<wire x1="7" y1="16" x2="7" y2="-16" width="0.127" layer="21"/>
<wire x1="7" y1="-16" x2="-7" y2="-16" width="0.127" layer="21"/>
<wire x1="-7" y1="-16" x2="-7" y2="16" width="0.127" layer="21"/>
<wire x1="-9" y1="17" x2="9" y2="17" width="0.6096" layer="21"/>
<wire x1="-9" y1="16" x2="9" y2="16" width="0.6096" layer="21"/>
<wire x1="-9" y1="15" x2="9" y2="15" width="0.6096" layer="21"/>
<wire x1="-9" y1="14" x2="9" y2="14" width="0.6096" layer="21"/>
<wire x1="-9" y1="13" x2="9" y2="13" width="0.6096" layer="21"/>
<wire x1="-9" y1="12" x2="9" y2="12" width="0.6096" layer="21"/>
<wire x1="-9" y1="9" x2="9" y2="9" width="0.6096" layer="21"/>
<wire x1="-9" y1="8" x2="9" y2="8" width="0.6096" layer="21"/>
<wire x1="-9" y1="6" x2="9" y2="6" width="0.6096" layer="21"/>
<wire x1="-9" y1="4" x2="9" y2="4" width="0.6096" layer="21"/>
<wire x1="-9" y1="2" x2="9" y2="2" width="0.6096" layer="21"/>
<wire x1="-9" y1="0" x2="9" y2="0" width="0.6096" layer="21"/>
<wire x1="-9" y1="-2" x2="9" y2="-2" width="0.6096" layer="21"/>
<wire x1="-9" y1="-4" x2="9" y2="-4" width="0.6096" layer="21"/>
<wire x1="-9" y1="-6" x2="9" y2="-6" width="0.6096" layer="21"/>
<wire x1="-9" y1="-8" x2="9" y2="-8" width="0.6096" layer="21"/>
<wire x1="-9" y1="-9" x2="9" y2="-9" width="0.6096" layer="21"/>
<wire x1="-9" y1="-12" x2="9" y2="-12" width="0.6096" layer="21"/>
<wire x1="-9" y1="-13" x2="9" y2="-13" width="0.6096" layer="21"/>
<wire x1="-9" y1="-14" x2="9" y2="-14" width="0.6096" layer="21"/>
<wire x1="-9" y1="-15" x2="9" y2="-15" width="0.6096" layer="21"/>
<wire x1="-9" y1="-16" x2="9" y2="-16" width="0.6096" layer="21"/>
<wire x1="-9" y1="-17" x2="9" y2="-17" width="0.6096" layer="21"/>
<pad name="1" x="-9" y="5" drill="0.8128" shape="long"/>
<pad name="2" x="9" y="5" drill="0.8128" shape="long"/>
<pad name="3" x="-9" y="-5" drill="0.8128" shape="long"/>
<pad name="4" x="9" y="-5" drill="0.8128" shape="long"/>
<text x="-10.16" y="-2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="12.7" y="-2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="11-33">
<description>R3311 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 18mm
(ØxB(W))[mm]: 38x18
manufactured by NKL®</description>
<wire x1="-6" y1="17" x2="6" y2="17" width="0.127" layer="21"/>
<wire x1="6" y1="17" x2="6" y2="-17" width="0.127" layer="21"/>
<wire x1="6" y1="-17" x2="-6" y2="-17" width="0.127" layer="21"/>
<wire x1="-6" y1="-17" x2="-6" y2="17" width="0.127" layer="21"/>
<wire x1="-7" y1="0" x2="7" y2="0" width="0.6096" layer="21"/>
<wire x1="-7" y1="2" x2="7" y2="2" width="0.6096" layer="21"/>
<wire x1="-7" y1="4" x2="7" y2="4" width="0.6096" layer="21"/>
<wire x1="-7" y1="6" x2="7" y2="6" width="0.6096" layer="21"/>
<wire x1="-7" y1="8" x2="7" y2="8" width="0.6096" layer="21"/>
<wire x1="-7" y1="11" x2="7" y2="11" width="0.6096" layer="21"/>
<wire x1="-7" y1="13" x2="7" y2="13" width="0.6096" layer="21"/>
<wire x1="-7" y1="14" x2="7" y2="14" width="0.6096" layer="21"/>
<wire x1="-7" y1="15" x2="7" y2="15" width="0.6096" layer="21"/>
<wire x1="-7" y1="16" x2="7" y2="16" width="0.6096" layer="21"/>
<wire x1="-7" y1="17" x2="7" y2="17" width="0.6096" layer="21"/>
<wire x1="-7" y1="18" x2="7" y2="18" width="0.6096" layer="21"/>
<wire x1="-7" y1="-2" x2="7" y2="-2" width="0.6096" layer="21"/>
<wire x1="-7" y1="-4" x2="7" y2="-4" width="0.6096" layer="21"/>
<wire x1="-7" y1="-6" x2="7" y2="-6" width="0.6096" layer="21"/>
<wire x1="-7" y1="-8" x2="7" y2="-8" width="0.6096" layer="21"/>
<wire x1="-7" y1="-11" x2="7" y2="-11" width="0.6096" layer="21"/>
<wire x1="-7" y1="-13" x2="7" y2="-13" width="0.6096" layer="21"/>
<wire x1="-7" y1="-14" x2="7" y2="-14" width="0.6096" layer="21"/>
<wire x1="-7" y1="-15" x2="7" y2="-15" width="0.6096" layer="21"/>
<wire x1="-7" y1="-17" x2="7" y2="-17" width="0.6096" layer="21"/>
<wire x1="-7" y1="-18" x2="7" y2="-18" width="0.6096" layer="21"/>
<wire x1="-7" y1="-16" x2="7" y2="-16" width="0.6096" layer="21"/>
<pad name="1" x="-9" y="0" drill="1.016" shape="long"/>
<pad name="2" x="9" y="0" drill="1.016" shape="long"/>
<text x="-7.62" y="2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="8.89" y="2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
</package>
<package name="10-24">
<description>R2408 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 9mm
(ØxH)[mm]: 29x12
manufactured by NKL®</description>
<wire x1="-12" y1="0" x2="-6" y2="0" width="0.6096" layer="21"/>
<wire x1="4" y1="0" x2="14" y2="0" width="0.6096" layer="21"/>
<wire x1="0" y1="4" x2="0" y2="14" width="0.6096" layer="21"/>
<wire x1="0" y1="-4" x2="0" y2="-14" width="0.6096" layer="21"/>
<wire x1="-4" y1="1" x2="-13.5" y2="2.5" width="0.6096" layer="21"/>
<wire x1="-4" y1="-1" x2="-13.5" y2="-2.5" width="0.6096" layer="21"/>
<wire x1="-3.5" y1="2" x2="-12.5" y2="5.5" width="0.6096" layer="21"/>
<wire x1="-3.5" y1="-2" x2="-12.5" y2="-5.5" width="0.6096" layer="21"/>
<wire x1="-3" y1="3" x2="-10" y2="9" width="0.6096" layer="21"/>
<wire x1="-3" y1="-3" x2="-10" y2="-9" width="0.6096" layer="21"/>
<wire x1="-1" y1="4" x2="-3.5" y2="13.5" width="0.6096" layer="21"/>
<wire x1="-1" y1="-4" x2="-3.5" y2="-13.5" width="0.6096" layer="21"/>
<wire x1="-2" y1="-3.5" x2="-7" y2="-11.5" width="0.6096" layer="21"/>
<wire x1="-2" y1="3.5" x2="-7" y2="11.5" width="0.6096" layer="21"/>
<wire x1="1" y1="-4" x2="3" y2="-13.5" width="0.6096" layer="21"/>
<wire x1="1" y1="4" x2="3" y2="13.5" width="0.6096" layer="21"/>
<wire x1="4" y1="1" x2="13.5" y2="3" width="0.6096" layer="21"/>
<wire x1="4" y1="-1" x2="13.5" y2="-3" width="0.6096" layer="21"/>
<wire x1="3.5" y1="2" x2="12.5" y2="5.5" width="0.6096" layer="21"/>
<wire x1="3.5" y1="-2" x2="12.5" y2="-5.5" width="0.6096" layer="21"/>
<wire x1="3" y1="3" x2="10" y2="9" width="0.6096" layer="21"/>
<wire x1="2" y1="3.5" x2="7" y2="11.5" width="0.6096" layer="21"/>
<wire x1="2" y1="-3.5" x2="7" y2="-12" width="0.6096" layer="21"/>
<wire x1="3" y1="-3" x2="10" y2="-9" width="0.6096" layer="21"/>
<wire x1="-13.5" y1="0" x2="-12" y2="0" width="0.6096" layer="51"/>
<wire x1="-6" y1="0" x2="-4.5" y2="0" width="0.6096" layer="51"/>
<circle x="0" y="0" radius="12" width="0.127" layer="21"/>
<circle x="0" y="0" radius="6" width="0.127" layer="21"/>
<pad name="1" x="-13.5" y="0" drill="1.016" shape="long"/>
<pad name="2" x="-4.5" y="0" drill="1.016" shape="long"/>
<text x="-2.54" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="10-27">
<description>R2711 - nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 9mm
(ØxH)[mm]: 25x12
manufactured by NKL®</description>
<wire x1="16" y1="0" x2="5" y2="0" width="0.6096" layer="21"/>
<wire x1="0" y1="5" x2="0" y2="16" width="0.6096" layer="21"/>
<wire x1="0" y1="-5" x2="0" y2="-16" width="0.6096" layer="21"/>
<wire x1="-5" y1="1" x2="-15.5" y2="3" width="0.6096" layer="21"/>
<wire x1="-5" y1="-1" x2="-15.5" y2="-3" width="0.6096" layer="21"/>
<wire x1="-4.5" y1="2" x2="-14.5" y2="6" width="0.6096" layer="21"/>
<wire x1="-4.5" y1="-2" x2="-15" y2="-6" width="0.6096" layer="21"/>
<wire x1="-4" y1="-3" x2="-13" y2="-9" width="0.6096" layer="21"/>
<wire x1="-4" y1="3" x2="-13" y2="9" width="0.6096" layer="21"/>
<wire x1="-3" y1="4" x2="-10.5" y2="12" width="0.6096" layer="21"/>
<wire x1="-10.5" y1="-12" x2="-3" y2="-4" width="0.6096" layer="21"/>
<wire x1="-1" y1="-5" x2="-3" y2="-15.5" width="0.6096" layer="21"/>
<wire x1="-1" y1="5" x2="-3" y2="15.5" width="0.6096" layer="21"/>
<wire x1="-2" y1="4.5" x2="-7" y2="14.5" width="0.6096" layer="21"/>
<wire x1="-7" y1="-14.5" x2="-2" y2="-4.5" width="0.6096" layer="21"/>
<wire x1="1" y1="5" x2="3" y2="15.5" width="0.6096" layer="21"/>
<wire x1="3" y1="-15.5" x2="1" y2="-5" width="0.6096" layer="21"/>
<wire x1="2" y1="4.5" x2="7" y2="14.5" width="0.6096" layer="21"/>
<wire x1="10.5" y1="12" x2="3" y2="4" width="0.6096" layer="21"/>
<wire x1="3" y1="-4" x2="10.5" y2="-12" width="0.6096" layer="21"/>
<wire x1="2" y1="-4.5" x2="7" y2="-14.5" width="0.6096" layer="21"/>
<wire x1="4" y1="-3" x2="13" y2="-9" width="0.6096" layer="21"/>
<wire x1="13" y1="9" x2="4" y2="3" width="0.6096" layer="21"/>
<wire x1="5" y1="1" x2="15.5" y2="3" width="0.6096" layer="21"/>
<wire x1="15.5" y1="-3" x2="5" y2="-1" width="0.6096" layer="21"/>
<wire x1="14.5" y1="6" x2="4.5" y2="2" width="0.6096" layer="21"/>
<wire x1="4.5" y1="-2" x2="14.5" y2="-6" width="0.6096" layer="21"/>
<wire x1="-14" y1="0" x2="-7" y2="0" width="0.6096" layer="21"/>
<wire x1="-16" y1="0" x2="-14" y2="0" width="0.6096" layer="51"/>
<wire x1="-7" y1="0" x2="-5" y2="0" width="0.6096" layer="51"/>
<circle x="0" y="0" radius="14" width="0.127" layer="21"/>
<circle x="0" y="0" radius="7" width="0.127" layer="21"/>
<pad name="2" x="-5" y="0" drill="1.016" shape="long"/>
<pad name="1" x="-16" y="0" drill="1.016" shape="long"/>
<text x="-2.54" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="10-33">
<description>R3311- nackte Drossel (plain choke)
ca. Maße (approx. dimensions):
RM (grid): 13mm
(ØxH)[mm]: 40x16
manufactured by NKL®</description>
<wire x1="-18" y1="0" x2="-9" y2="0" width="0.6096" layer="21"/>
<wire x1="8" y1="0" x2="19" y2="0" width="0.6096" layer="21"/>
<wire x1="0" y1="-8" x2="0" y2="-19" width="0.6096" layer="21"/>
<wire x1="0" y1="8" x2="0" y2="19" width="0.6096" layer="21"/>
<wire x1="8" y1="1" x2="18.5" y2="3" width="0.6096" layer="21"/>
<wire x1="8" y1="-1" x2="18.5" y2="-3" width="0.6096" layer="21"/>
<wire x1="7" y1="-4" x2="16.5" y2="-9" width="0.6096" layer="21"/>
<wire x1="7" y1="4" x2="16.5" y2="9" width="0.6096" layer="21"/>
<wire x1="-7" y1="4" x2="-16.5" y2="9" width="0.6096" layer="21"/>
<wire x1="-7" y1="-4" x2="-16.5" y2="-9" width="0.6096" layer="21"/>
<wire x1="7.5" y1="2.5" x2="18" y2="6" width="0.6096" layer="21"/>
<wire x1="7.5" y1="-2" x2="18" y2="-6" width="0.6096" layer="21"/>
<wire x1="-7.5" y1="2.5" x2="-18" y2="6" width="0.6096" layer="21"/>
<wire x1="-8" y1="1" x2="-18.5" y2="3" width="0.6096" layer="21"/>
<wire x1="-18.5" y1="-3" x2="-7.5" y2="-2" width="0.6096" layer="21"/>
<wire x1="-7.5" y1="-3" x2="-18" y2="-6" width="0.6096" layer="21"/>
<wire x1="1" y1="8" x2="3" y2="18.5" width="0.6096" layer="21"/>
<wire x1="-1" y1="8" x2="-3" y2="18.5" width="0.6096" layer="21"/>
<wire x1="1" y1="-8" x2="3" y2="-18.5" width="0.6096" layer="21"/>
<wire x1="-1" y1="-8" x2="-3" y2="-18.5" width="0.6096" layer="21"/>
<wire x1="4" y1="7" x2="9" y2="16.5" width="0.6096" layer="21"/>
<wire x1="-9" y1="16.5" x2="-4" y2="7" width="0.6096" layer="21"/>
<wire x1="-9" y1="-16.5" x2="-4" y2="-7" width="0.6096" layer="21"/>
<wire x1="9" y1="-16.5" x2="4" y2="-7" width="0.6096" layer="21"/>
<wire x1="-6" y1="-18" x2="-2.5" y2="-7.5" width="0.6096" layer="21"/>
<wire x1="6" y1="-18" x2="2.5" y2="-7.5" width="0.6096" layer="21"/>
<wire x1="6" y1="18" x2="2.5" y2="7.5" width="0.6096" layer="21"/>
<wire x1="-6.5" y1="18" x2="-2.5" y2="7.5" width="0.6096" layer="21"/>
<wire x1="-6.5" y1="-5" x2="-15" y2="-11.5" width="0.6096" layer="21"/>
<wire x1="-5.5" y1="-6" x2="-12" y2="-14.5" width="0.6096" layer="21"/>
<wire x1="5.5" y1="-6" x2="12" y2="-14.5" width="0.6096" layer="21"/>
<wire x1="6.5" y1="-5" x2="14.5" y2="-12" width="0.6096" layer="21"/>
<wire x1="5.5" y1="6" x2="12" y2="14.5" width="0.6096" layer="21"/>
<wire x1="6.5" y1="5" x2="14.5" y2="12" width="0.6096" layer="21"/>
<wire x1="-5.5" y1="6" x2="-12" y2="14.5" width="0.6096" layer="21"/>
<wire x1="-6.5" y1="5" x2="-14.5" y2="12" width="0.6096" layer="21"/>
<wire x1="-20" y1="0" x2="-18" y2="0" width="0.6096" layer="51"/>
<wire x1="-9" y1="0" x2="-7" y2="0" width="0.6096" layer="51"/>
<circle x="0" y="0" radius="17" width="0.127" layer="21"/>
<circle x="0" y="0" radius="10" width="0.127" layer="21"/>
<pad name="2" x="-7" y="0" drill="1.016" shape="long"/>
<pad name="1" x="-20" y="0" drill="1.016" shape="long"/>
<text x="-2.54" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B8">
<description>Becher B8 (cup B8)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 18x9
RM (grid) [mm]: 16
manufactured by NKL®</description>
<wire x1="-2.4" y1="8.675" x2="-2.4" y2="-8.675" width="0.127" layer="21" curve="149.056314"/>
<wire x1="2.4" y1="-8.675" x2="2.4" y2="8.675" width="0.127" layer="21" curve="149.056314"/>
<circle x="0" y="0" radius="9" width="0.127" layer="51"/>
<pad name="1" x="0" y="8" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="0" y="-8" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-2.54" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B60">
<description>Becher B60 (cup B60)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 53x31x55
RM (grid) [mm]: 22.5x30
manufactured by NKL®</description>
<wire x1="-27" y1="16" x2="27" y2="16" width="0.127" layer="21"/>
<wire x1="27" y1="16" x2="27" y2="-16" width="0.127" layer="21"/>
<wire x1="27" y1="-16" x2="-27" y2="-16" width="0.127" layer="21"/>
<wire x1="-27" y1="-16" x2="-27" y2="16" width="0.127" layer="21"/>
<pad name="5" x="0" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="6" x="0" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="3" x="-15" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="2" x="15" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="4" x="-15" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="1" x="15" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<text x="-17.78" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="3.81" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
<hole x="20" y="11.25" drill="2.54"/>
<hole x="20" y="-11.25" drill="2.54"/>
<hole x="-20" y="-11.25" drill="2.54"/>
<hole x="-20" y="11.25" drill="2.54"/>
<hole x="-25" y="0" drill="5.5"/>
<hole x="25" y="0" drill="5.5"/>
</package>
<package name="B19">
<description>Becher B19 (cup B19)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 18x13x20
RM (grid) [mm]: 10x5(x10/x15)</description>
<wire x1="9" y1="5" x2="9" y2="-5" width="0.127" layer="51"/>
<wire x1="9" y1="-5" x2="-9" y2="-5" width="0.127" layer="51"/>
<wire x1="-9" y1="-5" x2="-9" y2="5" width="0.127" layer="51"/>
<wire x1="9" y1="5" x2="-9" y2="5" width="0.127" layer="51"/>
<wire x1="1" y1="5" x2="4" y2="5" width="0.127" layer="51" curve="-180"/>
<wire x1="-4" y1="5" x2="-1" y2="5" width="0.127" layer="51" curve="-180"/>
<wire x1="-4" y1="-5" x2="-1" y2="-5" width="0.127" layer="51" curve="180"/>
<wire x1="1" y1="-5" x2="4" y2="-5" width="0.127" layer="51" curve="180"/>
<wire x1="6" y1="-5" x2="9" y2="-5" width="0.127" layer="51" curve="180"/>
<wire x1="-9" y1="-5" x2="-6" y2="-5" width="0.127" layer="51" curve="180"/>
<wire x1="-9" y1="5" x2="-6" y2="5" width="0.127" layer="51" curve="-180"/>
<wire x1="6" y1="5" x2="9" y2="5" width="0.127" layer="51" curve="-180"/>
<wire x1="-9" y1="-3.73" x2="-9" y2="3.73" width="0.127" layer="21"/>
<wire x1="9" y1="3.73" x2="9" y2="-3.73" width="0.127" layer="21"/>
<pad name="7" x="-2.5" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="6" x="2.5" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="5" x="7.5" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="8" x="-7.5" y="5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="1" x="-7.5" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="-2.5" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="2.5" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="7.5" y="-5" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-5.08" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B23">
<description>Becher B23 (cup B23)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 23x16x23
RM (grid) [mm]: 12.5x5(x10/x15/x20)
manufactured by NKL®</description>
<wire x1="-11" y1="6" x2="11" y2="6" width="0.127" layer="51"/>
<wire x1="11" y1="3.46" x2="11" y2="-3.46" width="0.127" layer="21"/>
<wire x1="11" y1="-6" x2="-11" y2="-6" width="0.127" layer="51"/>
<wire x1="-11" y1="-3.46" x2="-11" y2="3.46" width="0.127" layer="21"/>
<wire x1="-1.5" y1="6" x2="1.5" y2="6" width="0.127" layer="51" curve="-180"/>
<wire x1="-6.5" y1="6" x2="-3.5" y2="6" width="0.127" layer="51" curve="-180"/>
<wire x1="3.5" y1="6" x2="6.5" y2="6" width="0.127" layer="51" curve="-180"/>
<wire x1="-6.5" y1="-6" x2="-3.5" y2="-6" width="0.127" layer="51" curve="180"/>
<wire x1="-1.5" y1="-6" x2="1.5" y2="-6" width="0.127" layer="51" curve="180"/>
<wire x1="3.5" y1="-6" x2="6.5" y2="-6" width="0.127" layer="51" curve="180"/>
<wire x1="-11" y1="-5" x2="-8.5" y2="-6" width="0.127" layer="51" curve="223.602819"/>
<wire x1="8.5" y1="6" x2="11" y2="5" width="0.127" layer="51" curve="-223.602819"/>
<wire x1="-11" y1="5" x2="-8.5" y2="6" width="0.127" layer="51" curve="-223.602819"/>
<wire x1="8.5" y1="-6" x2="11" y2="-5" width="0.127" layer="51" curve="223.602819"/>
<wire x1="-10" y1="7.5" x2="10" y2="7.5" width="0.127" layer="51"/>
<wire x1="-10" y1="-7.5" x2="10" y2="-7.5" width="0.127" layer="51"/>
<wire x1="-11" y1="-6" x2="-11" y2="6" width="0.127" layer="51"/>
<wire x1="11" y1="6" x2="11" y2="-6" width="0.127" layer="51"/>
<pad name="8" x="0" y="6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="0" y="-6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="9" x="-5" y="6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="10" x="-10" y="6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="7" x="5" y="6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="6" x="10" y="6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="5" x="10" y="-6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="5" y="-6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="-5" y="-6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="1" x="-10" y="-6.25" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-6.35" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="0" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B60RP">
<description>Becher B60 (cup B60)  Rastpatent
top view, ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 53x31x55
RM (grid) [mm]: 22.5x30
manufactured by NKL®</description>
<wire x1="-27" y1="16" x2="27" y2="16" width="0.127" layer="21"/>
<wire x1="27" y1="16" x2="27" y2="-16" width="0.127" layer="21"/>
<wire x1="27" y1="-16" x2="-27" y2="-16" width="0.127" layer="21"/>
<wire x1="-27" y1="-16" x2="-27" y2="16" width="0.127" layer="21"/>
<pad name="1" x="0" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="2" x="0" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="3" x="-15" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="4" x="15" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="5" x="-15" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="6" x="15" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<text x="-17.78" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
<hole x="20" y="11.25" drill="2.54"/>
<hole x="20" y="-11.25" drill="2.54"/>
<hole x="-20" y="-11.25" drill="2.54"/>
<hole x="-20" y="11.25" drill="2.54"/>
<hole x="-25" y="0" drill="5.8"/>
<hole x="25" y="0" drill="5.8"/>
</package>
<package name="S60">
<description>Sockel S60 (base S60)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 53x31x55
RM (grid) [mm]: 22.5x30
manufactured by NKL®</description>
<wire x1="-25.5" y1="15" x2="25.5" y2="15" width="0.127" layer="21"/>
<wire x1="25.5" y1="15" x2="25.5" y2="-15" width="0.127" layer="21"/>
<wire x1="25.5" y1="-15" x2="-25.5" y2="-15" width="0.127" layer="21"/>
<wire x1="-25.5" y1="-15" x2="-25.5" y2="15" width="0.127" layer="21"/>
<pad name="5" x="0" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="6" x="0" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="3" x="-15" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="2" x="15" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="4" x="-15" y="-11.25" drill="1.4224" diameter="5" shape="octagon"/>
<pad name="1" x="15" y="11.25" drill="1.4224" diameter="5" shape="octagon"/>
<text x="-17.78" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="6.35" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
<hole x="20" y="11.25" drill="2.54"/>
<hole x="20" y="-11.25" drill="2.54"/>
<hole x="-20" y="-11.25" drill="2.54"/>
<hole x="-20" y="11.25" drill="2.54"/>
<hole x="-25" y="0" drill="5.5"/>
<hole x="25" y="0" drill="5.5"/>
</package>
<package name="S50">
<description>Sockel S50 (base S50)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 40x21x43
RM (grid) [mm]: 15x25
manufactured by NKL®</description>
<wire x1="-19.5" y1="10" x2="19.5" y2="10" width="0.127" layer="21"/>
<wire x1="19.5" y1="10" x2="19.5" y2="-10" width="0.127" layer="21"/>
<wire x1="19.5" y1="-10" x2="-19.5" y2="-10" width="0.127" layer="21"/>
<wire x1="-19.5" y1="-10" x2="-19.5" y2="10" width="0.127" layer="21"/>
<pad name="5" x="0" y="7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="6" x="0" y="-7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="1" x="12.5" y="7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="2" x="12.5" y="-7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="4" x="-12.5" y="-7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="3" x="-12.5" y="7.5" drill="1.016" diameter="3.81" shape="octagon"/>
<text x="-7.62" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="1.27" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-19" y="0" drill="4"/>
<hole x="19" y="0" drill="4"/>
</package>
<package name="S40">
<description>Sockel S40 (base S40)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 35x20x36
RM (grid) [mm]: 12.5x20
manufactured by NKL®</description>
<wire x1="-16.5" y1="9" x2="16.5" y2="9" width="0.127" layer="21"/>
<wire x1="16.5" y1="9" x2="16.5" y2="-9" width="0.127" layer="21"/>
<wire x1="16.5" y1="-9" x2="-16.5" y2="-9" width="0.127" layer="21"/>
<wire x1="-16.5" y1="-9" x2="-16.5" y2="9" width="0.127" layer="21"/>
<pad name="5" x="0" y="6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="6" x="0" y="-6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="1" x="10" y="6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="2" x="10" y="-6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="4" x="-10" y="-6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<pad name="3" x="-10" y="6.25" drill="1.016" diameter="3.81" shape="octagon"/>
<text x="-7.62" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="0" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-16" y="0" drill="4"/>
<hole x="16" y="0" drill="4"/>
</package>
<package name="S30">
<description>Sockel S30 (base S30)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 27x14x30
RM (grid) [mm]: 7.5x15
manufactured by NKL®</description>
<wire x1="-13" y1="6.5" x2="13" y2="6.5" width="0.127" layer="21"/>
<wire x1="13" y1="6.5" x2="13" y2="-6.5" width="0.127" layer="21"/>
<wire x1="13" y1="-6.5" x2="-13" y2="-6.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-6.5" x2="-13" y2="6.5" width="0.127" layer="21"/>
<pad name="5" x="0" y="3.75" drill="0.8128" diameter="2.54" shape="octagon"/>
<pad name="6" x="0" y="-3.75" drill="0.8128" diameter="2.54" shape="octagon"/>
<pad name="1" x="7.5" y="3.75" drill="0.8128" diameter="2.54" shape="octagon"/>
<pad name="2" x="7.5" y="-3.75" drill="0.8128" diameter="2.54" shape="octagon"/>
<pad name="4" x="-7.5" y="-3.75" drill="0.8128" diameter="2.54" shape="octagon"/>
<pad name="3" x="-7.5" y="3.75" drill="0.8128" diameter="2.54" shape="octagon"/>
<text x="-8.89" y="0" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.27" y="-1.27" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-12.5" y="0" drill="4"/>
<hole x="12.5" y="0" drill="4"/>
</package>
<package name="S10">
<description>Sockel S10 (base S10)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 18x10x21
RM (grid) [mm]: 5x10
manufactured by NKL®</description>
<wire x1="-8.5" y1="4.5" x2="8.5" y2="4.5" width="0.127" layer="21"/>
<wire x1="8.5" y1="4.5" x2="8.5" y2="-4.5" width="0.127" layer="21"/>
<wire x1="8.5" y1="-4.5" x2="-8.5" y2="-4.5" width="0.127" layer="21"/>
<wire x1="-8.5" y1="-4.5" x2="-8.5" y2="4.5" width="0.127" layer="21"/>
<pad name="5" x="0" y="2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="6" x="0" y="-2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="1" x="5" y="2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="2" x="5" y="-2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="4" x="-5" y="-2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<pad name="3" x="-5" y="2.5" drill="0.8128" diameter="2.1844" shape="octagon"/>
<text x="-7.62" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-1.27" size="1.27" layer="27">&gt;VALUE</text>
<hole x="-8" y="0" drill="3"/>
<hole x="8" y="0" drill="3"/>
</package>
<package name="SMD">
<description>SMD     top view
ca. Maße (approx. dim.)[mm]:
LxB(W)xH : 17x13x7
pad: 2.8x1.8</description>
<wire x1="-6.5" y1="8.5" x2="6.5" y2="8.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="8.5" x2="6.5" y2="-8.5" width="0.127" layer="21"/>
<wire x1="6.5" y1="-8.5" x2="-6.5" y2="-8.5" width="0.127" layer="21"/>
<wire x1="-6.5" y1="-8.5" x2="-6.5" y2="8.5" width="0.127" layer="21"/>
<smd name="4" x="-4.5" y="6.9" dx="1.8" dy="2.8" layer="1"/>
<smd name="3" x="-1.5" y="6.9" dx="1.8" dy="2.8" layer="1"/>
<smd name="2" x="1.5" y="6.9" dx="1.8" dy="2.8" layer="1"/>
<smd name="1" x="4.5" y="6.9" dx="1.8" dy="2.8" layer="1"/>
<smd name="5" x="-4.5" y="-6.9" dx="1.8" dy="2.8" layer="1"/>
<smd name="6" x="-1.5" y="-6.9" dx="1.8" dy="2.8" layer="1"/>
<smd name="7" x="1.5" y="-6.9" dx="1.8" dy="2.8" layer="1"/>
<smd name="8" x="4.5" y="-6.9" dx="1.8" dy="2.8" layer="1"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="S11-10">
<description>Sockel S11 (base S11)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 12x6x12
RM (grid) [mm]: 7.5
manufactured by NKL®</description>
<wire x1="-6" y1="3" x2="6" y2="3" width="0.127" layer="21"/>
<wire x1="6" y1="3" x2="6" y2="-3" width="0.127" layer="21"/>
<wire x1="6" y1="-3" x2="-6" y2="-3" width="0.127" layer="21"/>
<wire x1="-6" y1="-3" x2="-6" y2="3" width="0.127" layer="21"/>
<pad name="1" x="-3.75" y="0" drill="1.1" diameter="3" shape="octagon"/>
<pad name="2" x="3.75" y="0" drill="1.1" diameter="3" shape="octagon"/>
<text x="-2.54" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="S11-13">
<description>Sockel S11 (base S11)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 16x9x18
RM (grid) [mm]: 7.5
manufactured by NKL®</description>
<wire x1="-8" y1="4.5" x2="8" y2="4.5" width="0.127" layer="21"/>
<wire x1="8" y1="4.5" x2="8" y2="-4.5" width="0.127" layer="21"/>
<wire x1="8" y1="-4.5" x2="-8" y2="-4.5" width="0.127" layer="21"/>
<wire x1="-8" y1="-4.5" x2="-8" y2="4.5" width="0.127" layer="21"/>
<pad name="1" x="-3.75" y="0" drill="0.8128" diameter="3" shape="octagon"/>
<pad name="2" x="3.75" y="0" drill="0.8128" diameter="3" shape="octagon"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="S11-17">
<description>Sockel S11 (base S11)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 21x11x23
RM (grid) [mm]: 12.5
manufactured by NKL®</description>
<wire x1="-10.5" y1="5.5" x2="10.5" y2="5.5" width="0.127" layer="21"/>
<wire x1="10.5" y1="5.5" x2="10.5" y2="-5.5" width="0.127" layer="21"/>
<wire x1="10.5" y1="-5.5" x2="-10.5" y2="-5.5" width="0.127" layer="21"/>
<wire x1="-10.5" y1="-5.5" x2="-10.5" y2="5.5" width="0.127" layer="21"/>
<pad name="1" x="-6.25" y="0" drill="1.1" diameter="3" shape="octagon"/>
<pad name="2" x="6.25" y="0" drill="1.1" diameter="3" shape="octagon"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="S11-20">
<description>Sockel S11 (base S11)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 25x12x27
RM (grid) [mm]: 15
manufactured by NKL®</description>
<wire x1="-12.5" y1="6" x2="12.5" y2="6" width="0.127" layer="21"/>
<wire x1="12.5" y1="6" x2="12.5" y2="-6" width="0.127" layer="21"/>
<wire x1="12.5" y1="-6" x2="-12.5" y2="-6" width="0.127" layer="21"/>
<wire x1="-12.5" y1="-6" x2="-12.5" y2="6" width="0.127" layer="21"/>
<pad name="1" x="-7.5" y="0" drill="1.1" diameter="3.81" shape="octagon"/>
<pad name="2" x="7.5" y="0" drill="1.1" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="KS3615">
<description>Kappe KS3615 (case KS3615)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 46x23x43
RM (grid) [mm]: 17.5x20
manufactured by NKL®</description>
<wire x1="-12" y1="-12.5" x2="-12" y2="12.5" width="0.127" layer="21"/>
<wire x1="-12" y1="12.5" x2="12" y2="12.5" width="0.127" layer="21"/>
<wire x1="12" y1="12.5" x2="12" y2="-12.5" width="0.127" layer="21"/>
<wire x1="12" y1="-12.5" x2="-12" y2="-12.5" width="0.127" layer="21"/>
<wire x1="-13" y1="-23" x2="-13" y2="23" width="0.127" layer="21"/>
<wire x1="-13" y1="23" x2="13" y2="23" width="0.127" layer="21"/>
<wire x1="13" y1="23" x2="13" y2="-23" width="0.127" layer="21"/>
<wire x1="13" y1="-23" x2="-13" y2="-23" width="0.127" layer="21"/>
<pad name="1" x="-10" y="-8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="3" x="-10" y="8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="4" x="10" y="8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<pad name="2" x="10" y="-8.75" drill="1.27" diameter="3.81" shape="octagon"/>
<text x="-5.08" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.08" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B44(ST)">
<description>Becher B44 (cup B44)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 44x25(38)
RM (grid) [mm]: 37.5*15
manufactured by NKL®</description>
<circle x="0" y="0" radius="22" width="0.127" layer="21"/>
<pad name="1" x="-18.75" y="7.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="2" x="18.75" y="7.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="3" x="-18.75" y="-7.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="4" x="18.75" y="-7.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<text x="-2.54" y="6.35" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B2814">
<description>Becher B28 (cup B28)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 28x14
RM (grid) [mm]: 20*15 / 25
manufactured by NKL®</description>
<wire x1="-9.6" y1="10.2" x2="-9.6" y2="-10.2" width="0.127" layer="21" curve="93.471409"/>
<wire x1="-7.2" y1="-12" x2="-1.65" y2="-13.9" width="0.127" layer="21" curve="24.189514"/>
<wire x1="7.2" y1="-12" x2="1.65" y2="-13.9" width="0.127" layer="21" curve="-24.189695"/>
<wire x1="9.6" y1="-10.2" x2="9.6" y2="10.2" width="0.127" layer="21" curve="93.471409"/>
<wire x1="7.2" y1="12" x2="1.65" y2="13.9" width="0.127" layer="21" curve="24.189695"/>
<wire x1="-7.2" y1="12" x2="-1.65" y2="13.9" width="0.127" layer="21" curve="-24.189695"/>
<circle x="0" y="0" radius="14" width="0.127" layer="51"/>
<pad name="4" x="7.5" y="10" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="3" x="7.5" y="-10" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="2" x="-7.5" y="10" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="1" x="-7.5" y="-10" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="6" x="0" y="12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="5" x="0" y="-12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="5.08" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-6.35" size="1.27" layer="27">&gt;VALUE</text>
<hole x="0" y="0" drill="3"/>
</package>
<package name="B2818">
<description>Becher B2818 (cup B2818)   top view
ca. Maße (approx. dimensions):
LxBxH [mm]: 28x28x18
RM (grid) [mm]: 37.5*15
manufactured by NKL®</description>
<wire x1="-14" y1="14" x2="14" y2="14" width="0.127" layer="51"/>
<wire x1="14" y1="14" x2="14" y2="-14" width="0.127" layer="21"/>
<wire x1="14" y1="-14" x2="-14" y2="-14" width="0.127" layer="51"/>
<wire x1="-14" y1="-14" x2="-14" y2="14" width="0.127" layer="21"/>
<wire x1="-14" y1="14" x2="-9.2" y2="14" width="0.127" layer="21"/>
<wire x1="14" y1="-14" x2="9.2" y2="-14" width="0.127" layer="21"/>
<wire x1="-5.6" y1="14" x2="5.6" y2="14" width="0.127" layer="21"/>
<wire x1="9.2" y1="14" x2="14" y2="14" width="0.127" layer="21"/>
<wire x1="-9.2" y1="-14" x2="-14" y2="-14" width="0.127" layer="21"/>
<pad name="1" x="-7.5" y="12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="2" x="7.5" y="12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="3" x="-2.5" y="-12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="4" x="2.5" y="-12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="5" x="7.5" y="-12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="6" x="-7.5" y="-12.5" drill="0.8128" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B6Ø">
<description>Becher B60 (cup B60)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 60x34
RM (grid) [mm]: Ø10 + Ø22.5
manufactured by NKL®</description>
<circle x="0" y="0" radius="30" width="0.127" layer="21"/>
<pad name="1" x="-10" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="2" x="10" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="3" x="22.5" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="4" x="-22.5" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<text x="-6.35" y="10.16" size="1.27" layer="25">&gt;NAME</text>
<text x="-6.35" y="-11.43" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B70">
<description>Becher B70 (cup B70)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 70x45
RM (grid) [mm]: Ø12.5*Ø30
manufactured by NKL®</description>
<circle x="0" y="0" radius="35" width="0.127" layer="21"/>
<pad name="1" x="-12.5" y="0" drill="1.27" diameter="6.4516" shape="octagon"/>
<pad name="2" x="-30" y="0" drill="1.27" diameter="6.4516" shape="octagon"/>
<pad name="3" x="12.5" y="0" drill="1.27" diameter="6.4516" shape="octagon"/>
<pad name="4" x="30" y="0" drill="1.27" diameter="6.4516" shape="octagon"/>
<text x="-3.81" y="7.62" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-10.16" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B6">
<description>Becher B6 (cup B6)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 16x11
RM (grid) [mm]: 8.75x10 / 5x12.5
manufactured by NKL®</description>
<wire x1="-5.6" y1="5.7" x2="-5.6" y2="-5.7" width="0.127" layer="21" curve="91.014058"/>
<wire x1="-1.6" y1="-7.825" x2="1.6" y2="-7.825" width="0.127" layer="21" curve="23.076403"/>
<wire x1="5.6" y1="-5.7" x2="5.6" y2="5.7" width="0.127" layer="21" curve="91.014058"/>
<wire x1="1.6" y1="7.825" x2="-1.6" y2="7.825" width="0.127" layer="21" curve="23.076403"/>
<circle x="0" y="0" radius="8" width="0.127" layer="51"/>
<pad name="3" x="4.375" y="-5" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<pad name="1" x="-4.375" y="-5" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<pad name="2" x="-4.375" y="5" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<pad name="4" x="4.375" y="5" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<pad name="5" x="-2.5" y="-6.25" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<pad name="7" x="2.5" y="-6.25" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<pad name="6" x="-2.5" y="6.25" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<pad name="8" x="2.5" y="6.25" drill="1.27" diameter="1.6764" shape="long" rot="R90"/>
<text x="-2.54" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B9">
<description>Becher B9 (cup B9)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 18(20)x9
RM (grid) [mm]: 10x12.5 / 16
manufactured by NKL®</description>
<wire x1="-6" y1="7.375" x2="-6" y2="-7.375" width="0.127" layer="21" curve="101.739201"/>
<wire x1="-4.8" y1="-8.2" x2="-0.95" y2="-9.45" width="0.127" layer="21" curve="24.610398"/>
<wire x1="4.8" y1="-8.2" x2="0.95" y2="-9.45" width="0.127" layer="21" curve="-24.610127"/>
<wire x1="6" y1="-7.375" x2="6" y2="7.375" width="0.127" layer="21" curve="101.739201"/>
<wire x1="4.8" y1="8.2" x2="0.95" y2="9.45" width="0.127" layer="21" curve="24.610127"/>
<wire x1="-4.8" y1="8.2" x2="-0.95" y2="9.45" width="0.127" layer="21" curve="-24.610127"/>
<circle x="0" y="0" radius="9.5" width="0.127" layer="51"/>
<pad name="4" x="5" y="6.25" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="2" x="-5" y="6.25" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="1" x="-5" y="-6.25" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="3" x="5" y="-6.25" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="6" x="0" y="8" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<pad name="5" x="0" y="-8" drill="1.27" diameter="1.778" shape="long" rot="R90"/>
<text x="-2.54" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="B42">
<description>Becher B42 (cup B42)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 42x25/36
RM (grid) [mm]: 30x20 / 15 / 35
manufactured by NKL®</description>
<circle x="0" y="0" radius="21" width="0.127" layer="21"/>
<circle x="0" y="0" radius="2" width="0.127" layer="21"/>
<pad name="2" x="-15" y="10" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="3" x="15" y="-10" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="4" x="-15" y="-10" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="5" x="7.5" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="6" x="17.5" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="7" x="-7.5" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="8" x="-17.5" y="0" drill="0.8128" diameter="3.81" shape="octagon"/>
<pad name="1" x="15" y="10" drill="0.8128" diameter="3.81" shape="octagon"/>
<text x="-3.81" y="7.62" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-10.16" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="INDUCTOR-8X8MM" urn="urn:adsk.eagle:footprint:5829086/1">
<wire x1="-2.175" y1="-4.064" x2="-4.064" y2="-2.175" width="0.127" layer="51"/>
<wire x1="-4.064" y1="-2.175" x2="-4.064" y2="1.825" width="0.127" layer="51"/>
<wire x1="-4.064" y1="1.825" x2="-2.175" y2="4.064" width="0.127" layer="51"/>
<wire x1="-2.175" y1="4.064" x2="2.125" y2="4.064" width="0.127" layer="51"/>
<wire x1="2.125" y1="4.064" x2="4.064" y2="1.825" width="0.127" layer="51"/>
<wire x1="4.064" y1="1.825" x2="4.064" y2="-2.175" width="0.127" layer="51"/>
<wire x1="4.064" y1="-2.175" x2="2.125" y2="-4.064" width="0.127" layer="51"/>
<wire x1="2.125" y1="-4.064" x2="-2.175" y2="-4.064" width="0.127" layer="51"/>
<smd name="1" x="-2.794" y="0" dx="8.2042" dy="2.5908" layer="1" rot="R90"/>
<smd name="2" x="2.794" y="0" dx="8.2042" dy="2.5908" layer="1" rot="R90"/>
<text x="-2.905" y="5.095" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.905" y="-6.335" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="2200-12.7" urn="urn:adsk.eagle:footprint:25525/1">
<description>&lt;b&gt;newport components&lt;/b&gt; 2200 Serie RM 12.7 mm&lt;p&gt;
Miniatur Axial Lead Inductors&lt;br&gt;
Source: www.rsonline.de&lt;br&gt;
Order code 240-517</description>
<wire x1="-4.9" y1="1.9" x2="4.9" y2="1.9" width="0.2032" layer="51"/>
<wire x1="4.9" y1="1.9" x2="4.9" y2="-1.9" width="0.2032" layer="51"/>
<wire x1="4.9" y1="-1.9" x2="-4.9" y2="-1.9" width="0.2032" layer="51"/>
<wire x1="-4.9" y1="-1.9" x2="-4.9" y2="1.9" width="0.2032" layer="51"/>
<wire x1="-6.35" y1="0" x2="-5.08" y2="0" width="0.5" layer="51"/>
<wire x1="6.35" y1="0" x2="5.08" y2="0" width="0.5" layer="51"/>
<pad name="1" x="-6.35" y="0" drill="0.8" diameter="1.27"/>
<pad name="2" x="6.35" y="0" drill="0.8" diameter="1.27"/>
<text x="-4.445" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-0.635" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="INDUCTOR_L0603" urn="urn:adsk.eagle:footprint:7880077/1">
<wire x1="-1.397" y1="0.635" x2="1.397" y2="0.635" width="0.127" layer="21"/>
<wire x1="1.397" y1="0.635" x2="1.397" y2="-0.635" width="0.127" layer="21"/>
<wire x1="1.397" y1="-0.635" x2="-1.397" y2="-0.635" width="0.127" layer="21"/>
<wire x1="-1.397" y1="-0.635" x2="-1.397" y2="0.635" width="0.127" layer="21"/>
<smd name="1" x="-0.762" y="0" dx="0.889" dy="0.889" layer="1" roundness="25"/>
<smd name="2" x="0.762" y="0" dx="0.889" dy="0.889" layer="1" roundness="25"/>
<text x="-1.905" y="0.889" size="0.889" layer="25" ratio="11">&gt;NAME</text>
<text x="-1.905" y="-1.7145" size="0.889" layer="27" ratio="11">&gt;VALUE</text>
</package>
<package name="SM-1206" urn="urn:adsk.eagle:footprint:14558/1">
<description>SMD CHIP &lt;B&gt;INDUCTOR&lt;/B&gt;&lt;p&gt;
body 1206</description>
<wire x1="1.3" y1="0.7" x2="1.3" y2="0.6" width="0.2032" layer="51"/>
<wire x1="1.3" y1="0.6" x2="1.3" y2="-0.6" width="0.2032" layer="51"/>
<wire x1="1.3" y1="-0.6" x2="1.3" y2="-0.7" width="0.2032" layer="51"/>
<wire x1="1.3" y1="-0.7" x2="2.1" y2="-0.7" width="0.2032" layer="51"/>
<wire x1="2.1" y1="-0.7" x2="2.1" y2="0.7" width="0.2032" layer="51"/>
<wire x1="2.1" y1="0.7" x2="1.3" y2="0.7" width="0.2032" layer="51"/>
<wire x1="-2.1" y1="0.7" x2="-2.1" y2="-0.7" width="0.2032" layer="51"/>
<wire x1="-2.1" y1="-0.7" x2="-1.3" y2="-0.7" width="0.2032" layer="51"/>
<wire x1="-1.3" y1="-0.7" x2="-1.3" y2="-0.6" width="0.2032" layer="51"/>
<wire x1="-1.3" y1="-0.6" x2="-1.3" y2="0.6" width="0.2032" layer="51"/>
<wire x1="-1.3" y1="0.6" x2="-1.3" y2="0.7" width="0.2032" layer="51"/>
<wire x1="-1.3" y1="0.7" x2="-2.1" y2="0.7" width="0.2032" layer="51"/>
<wire x1="-1.3" y1="-0.6" x2="-0.9" y2="-0.6" width="0.2032" layer="51"/>
<wire x1="-0.9" y1="-0.6" x2="0.9" y2="-0.6" width="0.2032" layer="21"/>
<wire x1="0.9" y1="-0.6" x2="1.3" y2="-0.6" width="0.2032" layer="51"/>
<wire x1="1.3" y1="0.6" x2="0.9" y2="0.6" width="0.2032" layer="51"/>
<wire x1="0.9" y1="0.6" x2="-0.9" y2="0.6" width="0.2032" layer="21"/>
<wire x1="-0.9" y1="0.6" x2="-1.3" y2="0.6" width="0.2032" layer="51"/>
<smd name="1" x="-1.65" y="0" dx="1.2" dy="1.8" layer="1"/>
<smd name="2" x="1.65" y="0" dx="1.2" dy="1.8" layer="1"/>
<text x="-2.143" y="0.997" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.208" y="-2.308" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="INDUCTOR-8X8MM" urn="urn:adsk.eagle:package:5829529/4" type="model">
<packageinstances>
<packageinstance name="INDUCTOR-8X8MM"/>
</packageinstances>
</package3d>
<package3d name="2200-12.7" urn="urn:adsk.eagle:package:25963/2" type="model">
<description>newport components 2200 Serie RM 12.7 mm
Miniatur Axial Lead Inductors
Source: www.rsonline.de
Order code 240-517</description>
<packageinstances>
<packageinstance name="2200-12.7"/>
</packageinstances>
</package3d>
<package3d name="INDUCTOR_L0603" urn="urn:adsk.eagle:package:5829838/3" type="model">
<packageinstances>
<packageinstance name="INDUCTOR_L0603"/>
</packageinstances>
</package3d>
<package3d name="SM-1206" urn="urn:adsk.eagle:package:14693/2" type="model">
<description>SMD CHIP INDUCTOR
body 1206</description>
<packageinstances>
<packageinstance name="SM-1206"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="STROKO">
<wire x1="3.81" y1="1.016" x2="-3.81" y2="1.016" width="0.254" layer="94"/>
<wire x1="-3.81" y1="-1.016" x2="-3.81" y2="1.016" width="0.254" layer="94"/>
<wire x1="-3.81" y1="-1.016" x2="3.81" y2="-1.016" width="0.254" layer="94"/>
<circle x="-4.572" y="-3.302" radius="0.127" width="0.4064" layer="94"/>
<circle x="-4.572" y="1.778" radius="0.127" width="0.4064" layer="94"/>
<text x="-3.81" y="4.064" size="1.778" layer="95">&gt;NAME</text>
<text x="-3.81" y="-5.588" size="1.778" layer="96">&gt;VALUE</text>
<rectangle x1="-3.81" y1="1.651" x2="3.81" y2="3.429" layer="94"/>
<rectangle x1="-3.81" y1="-3.429" x2="3.81" y2="-1.651" layer="94"/>
<pin name="2" x="7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="1" x="-7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1"/>
<pin name="3" x="-7.62" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="2"/>
<pin name="4" x="7.62" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="2" rot="R180"/>
</symbol>
<symbol name="SINGLE">
<wire x1="-3.81" y1="1.651" x2="3.81" y2="1.651" width="0.254" layer="94"/>
<text x="-3.81" y="2.286" size="1.778" layer="95">&gt;NAME</text>
<text x="-3.937" y="-3.048" size="1.778" layer="96">&gt;VALUE</text>
<rectangle x1="-3.81" y1="-0.889" x2="3.81" y2="0.889" layer="94"/>
<pin name="2" x="7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="1" x="-7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1"/>
</symbol>
<symbol name="3*STROKO">
<wire x1="3.81" y1="1.016" x2="-3.81" y2="1.016" width="0.254" layer="94"/>
<wire x1="-3.81" y1="-1.016" x2="-3.81" y2="1.016" width="0.254" layer="94"/>
<wire x1="-3.81" y1="-1.016" x2="3.81" y2="-1.016" width="0.254" layer="94"/>
<wire x1="-3.81" y1="-6.096" x2="-3.81" y2="-4.064" width="0.254" layer="94"/>
<wire x1="3.81" y1="-4.064" x2="-3.81" y2="-4.064" width="0.254" layer="94"/>
<wire x1="-3.81" y1="-6.096" x2="3.81" y2="-6.096" width="0.254" layer="94"/>
<circle x="-4.572" y="-3.302" radius="0.127" width="0.4064" layer="94"/>
<circle x="-4.572" y="1.778" radius="0.127" width="0.4064" layer="94"/>
<circle x="-4.572" y="-8.382" radius="0.127" width="0.4064" layer="94"/>
<text x="-3.81" y="4.064" size="1.778" layer="95">&gt;NAME</text>
<text x="-3.81" y="-10.668" size="1.778" layer="96">&gt;VALUE</text>
<rectangle x1="-3.81" y1="1.651" x2="3.81" y2="3.429" layer="94"/>
<rectangle x1="-3.81" y1="-3.429" x2="3.81" y2="-1.651" layer="94"/>
<rectangle x1="-3.81" y1="-8.509" x2="3.81" y2="-6.731" layer="94"/>
<pin name="2" x="7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="1" x="-7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1"/>
<pin name="3" x="-7.62" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="2"/>
<pin name="4" x="7.62" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="2" rot="R180"/>
<pin name="5" x="-7.62" y="-7.62" visible="pad" length="middle" direction="pas" swaplevel="3"/>
<pin name="6" x="7.62" y="-7.62" visible="pad" length="middle" direction="pas" swaplevel="3" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="R1405X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B1" package="B1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B2" package="B2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B71" package="B71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B1/2" package="B1/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS1405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B10" package="B10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B19" package="B19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S10" package="S10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B9" package="B9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1405U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B1" package="B1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B1/2" package="B1/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B2" package="B2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B71" package="B71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS1405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B10" package="B10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B19" package="B19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S10" package="S10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B9" package="B9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1305F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B1" package="B1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B1/2" package="B1/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B71" package="B71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B10" package="B10">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B8" package="B8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S10" package="S10">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B9" package="B9">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1305D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B1" package="B1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B1/2" package="B1/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B71" package="B71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B10" package="B10">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B8" package="B8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S10" package="S10">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B9" package="B9">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1908X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B3" package="B3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS1908">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B30" package="B30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B2814" package="B2814">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2610X" prefix="L">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B4" package="B4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B40" package="B40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS2610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B34" package="B34">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S40" package="S40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R3213X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B50" package="B50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS3213">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S40" package="S40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B44" package="B44(ST)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1908U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B3" package="B3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS1908">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B30" package="B30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B2814" package="B2814">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2610U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B4" package="B4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B40" package="B40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS2610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B34" package="B34">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S40" package="S40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R3213U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B50" package="B50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS3213">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S40" package="S40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B44" package="B44(ST)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1705F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B2" package="B2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B23" package="B23">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2006F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B3" package="B3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B30" package="B30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B2814" package="B2814">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2408F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B4" package="B4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B40" package="B40">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2711F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B4" package="B4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B40" package="B40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B34" package="B34">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S40" package="S40">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R3311F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B50" package="B50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B44" package="B44">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-33">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-33">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B42" package="B42">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1705D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B2" package="B2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B23" package="B23">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2006D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B3" package="B3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B30" package="B30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B2814" package="B2814">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2408D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B4" package="B4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B40" package="B40">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R2711D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B4" package="B4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B40" package="B40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B34" package="B34">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S40" package="S40">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R3311D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B50" package="B50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B44" package="B44">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="10" package="10-33">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="11" package="11-33">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B42" package="B42">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1607X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B23" package="B23">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="9"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S30" package="S30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R4218X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="B60" package="B60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R5618X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B70" package="B70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R5618U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B70" package="B70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R4014F" prefix="L">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B60" package="B60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R4014D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B60" package="B60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R4718D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B60" package="B6Ø">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R5114D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B60" package="B6Ø">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R5814D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B70" package="B70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R4718F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B60" package="B6Ø">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R5114F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B60" package="B6Ø">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R5814F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="S60" package="S60">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B70" package="B70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1003U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="-SMD" package="SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B5" package="B5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS1003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B6" package="B6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1003X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="-SMD" package="SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B5" package="B5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="KS" package="KS1003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B6" package="B6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1003D" prefix="L" uservalue="yes">
<description>Speicherdrossel (bis typ. 250kHz)
storage choke (up to typ. 250kHz)</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="B5" package="B5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="-SMD" package="SMD">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B6" package="B6">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1003F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE" x="0" y="0"/>
</gates>
<devices>
<device name="-SMD" package="SMD">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B5" package="B5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B6" package="B6">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1303X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="KS" package="KS1303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1303U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="KS" package="KS1303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1003V" prefix="L" uservalue="yes">
<description>Übertrager (verlustarm) bis typ. 400kHz
Power transformer (low loss) up to typ. 400kHz</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="KS" package="KS1003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="-SMD" package="SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B5" package="B5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B6" package="B6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1303V" prefix="L" uservalue="yes">
<description>Übertrager (verlustarm) bis typ. 400kHz
Power transformer (low loss) up to typ. 400kHz</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="KS" package="KS1303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1405V" prefix="L" uservalue="yes">
<description>Übertrager (verlustarm) bis typ. 400kHz
Power transformer (low loss) up to typ. 400kHz</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="KS" package="KS1405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B1" package="B1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B10" package="B10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B1/2" package="B1/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B19" package="B19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B2" package="B2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="S10" package="S10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B71" package="B71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B9" package="B9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R3615X" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (bis typ. 10MHz)
common mode choke (up to typ. 10MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B50" package="B5Ø">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B60" package="B60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R3615U" prefix="L" uservalue="yes">
<description>Gleichtakt-Entstördrossel (über typ. 5MHz)
common mode choke (above typ.5MHz)</description>
<gates>
<gate name="G$1" symbol="STROKO" x="0" y="0"/>
</gates>
<devices>
<device name="S50" package="S50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B60" package="B60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
<device name="B50" package="B5Ø">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
<compatibility>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports URNs for individual library
assets (packages, symbols, and devices). The URNs of those assets
will not be understood (or retained) with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports the association of 3D packages
with devices in libraries, schematics, and board files. Those 3D
packages will not be understood (or retained) with this version.
</note>
</compatibility>
</eagle>
