<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting keepoldvectorfont="yes"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.1" unitdist="inch" unit="inch" style="lines" multiple="1" display="no" altdistance="0.01" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="90" name="Modules" color="5" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="no" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
</layers>
<library>
<description>&lt;LP38693MP-ADJ/NOPB, Low Dropout Voltage Regulator, Adjustable 0.5A, 1.25  9 V +/-2%, 5-Pin SOT-223&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT150P700X180-5N">
<description>&lt;b&gt;NDC0005A&lt;/b&gt;&lt;br&gt;
</description>
<smd name="1" x="-3.05" y="2.25" dx="1.9" dy="0.9" layer="1"/>
<smd name="2" x="-3.05" y="0.75" dx="1.9" dy="0.9" layer="1"/>
<smd name="3" x="-3.05" y="-0.75" dx="1.9" dy="0.9" layer="1"/>
<smd name="4" x="-3.05" y="-2.25" dx="1.9" dy="0.9" layer="1"/>
<smd name="5" x="3.05" y="0" dx="3.2" dy="1.9" layer="1" rot="R90"/>
<text x="-0.127" y="-4.318" size="1.27" layer="25" align="center">&gt;NAME</text>
<text x="-0.127" y="4.318" size="1.27" layer="27" align="center">&gt;VALUE</text>
<wire x1="-1.755" y1="3.25" x2="1.755" y2="3.25" width="0.1" layer="51"/>
<wire x1="1.755" y1="3.25" x2="1.755" y2="-3.25" width="0.1" layer="51"/>
<wire x1="1.755" y1="-3.25" x2="-1.755" y2="-3.25" width="0.1" layer="51"/>
<wire x1="-1.755" y1="-3.25" x2="-1.755" y2="3.25" width="0.1" layer="51"/>
<wire x1="-1.755" y1="1.75" x2="-0.255" y2="3.25" width="0.1" layer="51"/>
<wire x1="-1.75" y1="3.25" x2="1.75" y2="3.25" width="0.2" layer="21"/>
<wire x1="1.75" y1="3.25" x2="1.75" y2="-3.25" width="0.2" layer="21"/>
<wire x1="1.75" y1="-3.25" x2="-1.75" y2="-3.25" width="0.2" layer="21"/>
<wire x1="-1.75" y1="-3.25" x2="-1.75" y2="3.25" width="0.2" layer="21"/>
</package>
<package name="SOT223" urn="urn:adsk.eagle:footprint:28695/1">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
<wire x1="3.2766" y1="1.778" x2="3.2766" y2="-1.778" width="0.2032" layer="21"/>
<wire x1="3.2766" y1="-1.778" x2="-3.2766" y2="-1.778" width="0.2032" layer="21"/>
<wire x1="-3.2766" y1="-1.778" x2="-3.2766" y2="1.778" width="0.2032" layer="21"/>
<wire x1="-3.2766" y1="1.778" x2="3.2766" y2="1.778" width="0.2032" layer="21"/>
<smd name="1" x="-2.3114" y="-3.0988" dx="1.2192" dy="2.2352" layer="1"/>
<smd name="2" x="0" y="-3.0988" dx="1.2192" dy="2.2352" layer="1"/>
<smd name="3" x="2.3114" y="-3.0988" dx="1.2192" dy="2.2352" layer="1"/>
<smd name="4" x="0" y="3.099" dx="3.6" dy="2.2" layer="1"/>
<text x="1.0208" y="-4.318" size="0.8128" layer="21" ratio="12">3</text>
<text x="1.905" y="2.54" size="0.8128" layer="21" ratio="12">4</text>
<text x="-3.4526" y="-4.318" size="0.8128" layer="21" ratio="12">1</text>
<text x="-1.2906" y="-4.3274" size="0.8128" layer="21" ratio="12">2</text>
<text x="-2.54" y="0.0508" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-1.3208" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-1.6002" y1="1.8034" x2="1.6002" y2="3.6576" layer="51"/>
<rectangle x1="-0.4318" y1="-3.6576" x2="0.4318" y2="-1.8034" layer="51"/>
<rectangle x1="-2.7432" y1="-3.6576" x2="-1.8796" y2="-1.8034" layer="51"/>
<rectangle x1="1.8796" y1="-3.6576" x2="2.7432" y2="-1.8034" layer="51"/>
<rectangle x1="-1.6002" y1="1.8034" x2="1.6002" y2="3.6576" layer="51"/>
<rectangle x1="-0.4318" y1="-3.6576" x2="0.4318" y2="-1.8034" layer="51"/>
<rectangle x1="-2.7432" y1="-3.6576" x2="-1.8796" y2="-1.8034" layer="51"/>
<rectangle x1="1.8796" y1="-3.6576" x2="2.7432" y2="-1.8034" layer="51"/>
</package>
<package name="SOT230P700X180-5N" urn="urn:adsk.eagle:footprint:13315956/1">
<description>5-SOT223, 2.30 mm pitch, 7.00 mm span, 6.50 X 3.50 X 1.80 mm body
&lt;p&gt;5-pin SOT223 package with 2.30 mm pitch, 7.00 mm span with body size 6.50 X 3.50 X 1.80 mm&lt;/p&gt;</description>
<circle x="-2.9276" y="4.3986" radius="0.25" width="0" layer="21"/>
<wire x1="-1.85" y1="4.2086" x2="1.85" y2="4.2086" width="0.12" layer="21"/>
<wire x1="1.85" y1="4.2086" x2="1.85" y2="1.8486" width="0.12" layer="21"/>
<wire x1="-1.85" y1="-4.2086" x2="1.85" y2="-4.2086" width="0.12" layer="21"/>
<wire x1="1.85" y1="-4.2086" x2="1.85" y2="-1.8486" width="0.12" layer="21"/>
<wire x1="1.85" y1="-3.35" x2="-1.85" y2="-3.35" width="0.12" layer="51"/>
<wire x1="-1.85" y1="-3.35" x2="-1.85" y2="3.35" width="0.12" layer="51"/>
<wire x1="-1.85" y1="3.35" x2="1.85" y2="3.35" width="0.12" layer="51"/>
<wire x1="1.85" y1="3.35" x2="1.85" y2="-3.35" width="0.12" layer="51"/>
<smd name="1" x="-3.0226" y="3.45" dx="1.9651" dy="0.8891" layer="1"/>
<smd name="2" x="-3.0226" y="1.15" dx="1.9651" dy="0.8891" layer="1"/>
<smd name="3" x="-3.0226" y="-1.15" dx="1.9651" dy="0.8891" layer="1"/>
<smd name="4" x="-3.0226" y="-3.45" dx="1.9651" dy="0.8891" layer="1"/>
<smd name="5" x="3.0226" y="0" dx="1.9651" dy="3.1891" layer="1"/>
<text x="0" y="5.2836" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-4.8436" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SOT150P695X180-5M" urn="urn:adsk.eagle:footprint:13316036/1">
<description>5-SOT223, 1.50 mm pitch, 6.95 mm span, 6.55 X 3.50 X 1.80 mm body
&lt;p&gt;5-pin SOT223 package with 1.50 mm pitch, 6.95 mm span with body size 6.55 X 3.50 X 1.80 mm&lt;/p&gt;</description>
<circle x="-3.0031" y="3.2186" radius="0.25" width="0" layer="21"/>
<wire x1="-1.85" y1="2.9686" x2="-1.85" y2="3.35" width="0.12" layer="21"/>
<wire x1="-1.85" y1="3.35" x2="1.85" y2="3.35" width="0.12" layer="21"/>
<wire x1="1.85" y1="3.35" x2="1.85" y2="1.8686" width="0.12" layer="21"/>
<wire x1="-1.85" y1="-2.9686" x2="-1.85" y2="-3.35" width="0.12" layer="21"/>
<wire x1="-1.85" y1="-3.35" x2="1.85" y2="-3.35" width="0.12" layer="21"/>
<wire x1="1.85" y1="-3.35" x2="1.85" y2="-1.8686" width="0.12" layer="21"/>
<wire x1="1.85" y1="-3.35" x2="-1.85" y2="-3.35" width="0.12" layer="51"/>
<wire x1="-1.85" y1="-3.35" x2="-1.85" y2="3.35" width="0.12" layer="51"/>
<wire x1="-1.85" y1="3.35" x2="1.85" y2="3.35" width="0.12" layer="51"/>
<wire x1="1.85" y1="3.35" x2="1.85" y2="-3.35" width="0.12" layer="51"/>
<smd name="1" x="-3.0442" y="2.25" dx="2.224" dy="0.9291" layer="1"/>
<smd name="2" x="-3.0442" y="0.75" dx="2.224" dy="0.9291" layer="1"/>
<smd name="3" x="-3.0442" y="-0.75" dx="2.224" dy="0.9291" layer="1"/>
<smd name="4" x="-3.0442" y="-2.25" dx="2.224" dy="0.9291" layer="1"/>
<smd name="5" x="3.0442" y="0" dx="2.224" dy="3.2291" layer="1"/>
<text x="0" y="4.1036" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-3.985" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="SOT223" urn="urn:adsk.eagle:package:28758/2" type="model">
<description>Small Outline Transistor</description>
<packageinstances>
<packageinstance name="SOT223"/>
</packageinstances>
</package3d>
<package3d name="SOT150P695X180-5M" urn="urn:adsk.eagle:package:13316025/1" type="model">
<description>5-SOT223, 1.50 mm pitch, 6.95 mm span, 6.55 X 3.50 X 1.80 mm body
&lt;p&gt;5-pin SOT223 package with 1.50 mm pitch, 6.95 mm span with body size 6.55 X 3.50 X 1.80 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SOT150P695X180-5M"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="LP38693MP-ADJ_NOPB">
<wire x1="5.08" y1="2.54" x2="27.94" y2="2.54" width="0.254" layer="94"/>
<wire x1="27.94" y1="-7.62" x2="27.94" y2="2.54" width="0.254" layer="94"/>
<wire x1="27.94" y1="-7.62" x2="5.08" y2="-7.62" width="0.254" layer="94"/>
<wire x1="5.08" y1="2.54" x2="5.08" y2="-7.62" width="0.254" layer="94"/>
<text x="29.21" y="7.62" size="1.778" layer="95" align="center-left">&gt;NAME</text>
<text x="29.21" y="5.08" size="1.778" layer="96" align="center-left">&gt;VALUE</text>
<pin name="VEN" x="0" y="0" length="middle"/>
<pin name="ADJ" x="0" y="-2.54" length="middle"/>
<pin name="VOUT" x="0" y="-5.08" length="middle" direction="out"/>
<pin name="VIN" x="33.02" y="0" length="middle" direction="in" rot="R180"/>
<pin name="GND_TAB" x="33.02" y="-2.54" length="middle" direction="pwr" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LP38693MP-ADJ_NOPB" prefix="IC">
<description>&lt;b&gt;LP38693MP-ADJ/NOPB, Low Dropout Voltage Regulator, Adjustable 0.5A, 1.25  9 V +/-2%, 5-Pin SOT-223&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/lp38693-adj.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LP38693MP-ADJ_NOPB" x="0" y="0"/>
</gates>
<devices>
<device name="" package="SOT150P700X180-5N">
<connects>
<connect gate="G$1" pin="ADJ" pad="2"/>
<connect gate="G$1" pin="GND_TAB" pad="5"/>
<connect gate="G$1" pin="VEN" pad="1"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="LP38693MP-ADJ/NOPB, Low Dropout Voltage Regulator, Adjustable 0.5A, 1.25  9 V +/-2%, 5-Pin SOT-223" constant="no"/>
<attribute name="HEIGHT" value="1.8mm" constant="no"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments" constant="no"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LP38693MP-ADJ/NOPB" constant="no"/>
<attribute name="MOUSER_PART_NUMBER" value="926-LP38693MPADJNOPB" constant="no"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=926-LP38693MPADJNOPB" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693_2">
<gates>
<gate name="G$1" symbol="LP38693MP-ADJ_NOPB" x="-15.24" y="2.54"/>
</gates>
<devices>
<device name="" package="SOT150P695X180-5M">
<connects>
<connect gate="G$1" pin="ADJ" pad="2"/>
<connect gate="G$1" pin="GND_TAB" pad="5"/>
<connect gate="G$1" pin="VEN" pad="1"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13316025/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
<compatibility>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports URNs for individual library
assets (packages, symbols, and devices). The URNs of those assets
will not be understood (or retained) with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports the association of 3D packages
with devices in libraries, schematics, and board files. Those 3D
packages will not be understood (or retained) with this version.
</note>
</compatibility>
</eagle>
